{"text_format":"1","workbook":"xlsx","n_sheets":5,"sheets":["MI","Graph MI","LC","Graph LC","CO2"],"not_rendered":{"charts":18,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"MI","index":0,"n_rows":156,"n_cols":27,"rows_kept":156,"cut":false,"hidden":false,"merged":[[0,22,0,24],[1,22,1,24],[49,22,49,24],[50,22,50,24],[109,22,109,24],[110,22,110,24],[0,25,0,26],[49,25,49,26],[109,25,109,26],[0,4,0,6],[0,7,0,9],[0,10,0,12],[0,13,0,15],[0,16,0,18],[0,19,0,21],[6,0,9,0],[10,0,12,0],[13,0,16,0],[1,19,1,21],[59,0,61,0],[62,0,65,0],[115,0,118,0],[119,0,121,0],[122,0,125,0],[84,0,87,0],[35,0,38,0],[148,0,151,0],[144,0,147,0],[148,1,151,1],[148,2,148,3],[149,2,149,3],[150,2,150,3],[151,2,151,3],[140,1,143,1],[140,2,140,3],[141,2,141,3],[142,2,142,3],[143,2,143,3],[144,1,144,3],[145,1,145,3],[146,1,146,3],[147,1,147,3],[132,1,139,1],[132,2,132,3],[133,2,133,3],[134,2,134,3],[135,2,135,3],[136,2,136,3],[137,2,137,3],[138,2,138,3],[139,2,139,3],[129,1,129,3],[130,1,131,1],[130,2,130,3],[131,2,131,3],[122,1,125,1],[122,2,122,3],[123,2,123,3],[124,2,124,3],[125,2,125,3],[126,1,126,3],[110,10,110,12],[112,1,112,3],[113,1,113,3],[114,1,114,3],[115,1,118,1],[115,2,115,3],[88,0,91,0],[88,1,91,1],[88,2,88,3],[89,2,89,3],[90,2,90,3],[91,2,91,3],[116,2,116,3],[117,2,117,3],[118,2,118,3],[119,1,121,1],[119,2,119,3],[120,2,120,3],[121,2,121,3],[110,4,110,6],[110,7,110,9],[127,1,127,3],[128,1,128,3],[80,1,83,1],[80,2,80,3],[81,2,81,3],[82,2,82,3],[83,2,83,3],[84,1,84,3],[85,1,85,3],[86,1,86,3],[87,1,87,3],[96,1,96,2],[72,1,79,1],[72,2,72,3],[73,2,73,3],[74,2,74,3],[75,2,75,3],[76,2,76,3],[77,2,77,3],[78,2,78,3],[79,2,79,3],[54,1,54,3],[55,1,58,1],[55,2,55,3],[39,0,42,0],[39,1,42,1],[39,2,39,3],[40,2,40,3],[41,2,41,3],[42,2,42,3],[56,2,56,3],[57,2,57,3],[58,2,58,3],[55,0,58,0],[59,1,61,1],[59,2,59,3],[60,2,60,3],[61,2,61,3],[50,4,50,6],[50,7,50,9],[67,1,67,3],[68,1,68,3],[31,1,34,1],[31,2,31,3],[32,2,32,3],[33,2,33,3],[34,2,34,3],[35,1,35,3],[36,1,36,3],[37,1,37,3],[38,1,38,3],[63,2,63,3],[64,2,64,3],[65,2,65,3],[66,1,66,3],[49,7,49,9],[52,1,52,3],[53,1,53,3],[23,1,30,1],[23,2,23,3],[24,2,24,3],[25,2,25,3],[26,2,26,3],[27,2,27,3],[28,2,28,3],[29,2,29,3],[30,2,30,3],[21,1,22,1],[21,2,21,3],[22,2,22,3],[13,1,16,1],[13,2,13,3],[14,2,14,3],[15,2,15,3],[16,2,16,3],[17,1,17,3],[110,13,110,15],[110,16,110,18],[110,19,110,21],[1,10,1,12],[3,1,3,3],[4,1,4,3],[5,1,5,3],[6,1,9,1],[6,2,6,3],[1,13,1,15],[1,16,1,18],[7,2,7,3],[8,2,8,3],[9,2,9,3],[10,1,12,1],[10,2,10,3],[11,2,11,3],[12,2,12,3],[1,4,1,6],[1,7,1,9],[49,4,49,6],[18,1,18,3],[19,1,19,3],[20,1,20,3],[152,0,155,0],[152,1,155,1],[152,2,152,3],[153,2,153,3],[154,2,154,3],[155,2,155,3],[43,0,46,0],[43,1,46,1],[43,2,43,3],[44,2,44,3],[45,2,45,3],[46,2,46,3],[92,0,95,0],[92,1,95,1],[92,2,92,3],[93,2,93,3],[94,2,94,3],[95,2,95,3],[69,1,69,3],[70,1,71,1],[70,2,70,3],[71,2,71,3],[62,1,65,1],[62,2,62,3],[49,13,49,15],[49,16,49,18],[49,19,49,21],[109,4,109,6],[109,7,109,9],[109,10,109,12],[109,13,109,15],[109,16,109,18],[109,19,109,21],[50,13,50,15],[50,16,50,18],[50,19,50,21],[50,10,50,12],[49,10,49,12]]}
[null,null,null,null,"Gaz + CESI",null,null,"Gaz + CET",null,null,"PAC air/air + EJ +CET",null,null,"Bois + EJ + CET",null,null,"PAC DS air/eau ",null,null,"PAC DS air/eau + DF",null,null,"PAC DS air/eau + DF avec bypass",null,null,"PAC TS air/eau"]
["H1a",null,null,null,"V1",null,null,"V3",null,null,"V4_ssPV",null,null,"V5",null,null,"V6",null,null,"V7_DF",null,null,"V7_DF_BP",null,null,"V8 (EER=3.5 / Vt=-1.8K)","V8bis (EER=3 / Vt=0K)"]
[null,null,"Résultats - ENERGIE",null,"V1_Bbio_H1a","V1_Bbio20_H1a","V1_Bbio40_H1a","V3_Bbio_H1a","V3_Bbio20_H1a","V3_Bbio40_H1a","V4_Bbio_H1a","V4_Bbio20_H1a","V4_Bbio40_H1a","V5_Bbio_H1a","V5_Bbio20_H1a","V5_Bbio40_H1a","V6_Bbio_H1a","V6_Bbio20_H1a","V6_Bbio40_H1a","V7DF_Bbio_H1a","V7DF_Bbio20_H1a","V7DF_Bbio40_H1a","V7DF_Bbio_H1a","V7DF_Bbio20_H1a","V7DF_Bbio40_H1a","V8_Bbio20_H1a","V8bis_Bbio20_H1a"]
[null,"Cep (kWh/m2.an) H1a",null,null,62.9616157860005,56.2309176758897,48.487628705098899,71.716788306935996,64.902642771671694,57.012419623855699,85.329708637715598,75.944879931519495,65.593195500994,106.043697462068,92.768284427073596,77.1974122385746,64.163917716584095,59.642187650167301,54.377398986722802,72.288183267309705,67.762725479587502,62.6410823159556,null,67.485139198344498,null,58.0986223122204,55.869676068122303]
[null,"Cep_nr (kWh/m2SREF par an)",null,null,62.9616157860005,56.2309176758897,48.487628705098899,71.716788306935996,64.902642771671694,57.012419623855699,85.329708637715598,75.944879931519495,65.593195500994,62.898640426422702,57.904657078141099,51.793357810945501,64.163917716584095,59.642187650167301,54.377398986722802,72.288183267309705,67.762725479587502,62.6410823159556,null,67.485139198344498,null,58.0986223122204,55.869676068122303]
[null,"RCR (%)",null,null,0.131395653690564,0.13606661660121999,0.15224245232816799,9.5621225137298899E-2,9.7343598081009605E-2,0.100923327615192,0.13191639305484701,0.126290642062234,0.119182732781868,0.414715981155103,0.39058084270073901,0.35570853842605799,0.26514941378152601,0.23316477383582199,0.19279404451059601,0.41092610887077902,0.40483538423368798,0.39989846635337201,null,0.40008504389454702,null,0.16456636535731201,0.195912303116695]
["CH","Quantités d'énergie finale importées pour le chauffage (kWh/m2SREF)","Gaz",null,37.316610616250003,29.8586031799056,0,37.070011853289401,29.619853197573899,21.4703369064556,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Bois",null,0,0,0,0,0,0,0,0,0,43.145057035645699,34.863627348932397,25.404054427629099,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Reseau",null,0,0,0.18121339733714001,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Elec importée",null,0.235339391373907,0.21016622468715601,0,0.236324238037106,0.21110963733457599,0.182090918372637,22.941149565125599,18.498728927222199,13.761664153521,13.202020860919699,10.667973741874301,7.7734248034116602,11.8590181492543,9.5707670554138602,7.1038867846201903,12.881689827333499,10.6441500384754,8.1037251783052699,null,10.644124139466401,null,9.5707670556135405,9.5841540028584902]
["FR","Quantités d'énergie finale importées pour le refroidissement (kWh/m2SREF)","Gaz",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Reseau",null,0,0,4.0252527142654602,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Elec importée",null,3.4256072178391102,3.7884471427867101,0,3.4256072178391102,3.7884471427867101,4.0252527142654602,3.4256072178391102,3.7884471427867101,4.0252527142654602,3.4256072178391102,3.7884471427867101,4.0252527142654504,3.4256072178391102,3.7884471427867101,4.0252527142650001,3.8185085964528702,4.1331200548169198,4.5348313846518398,null,4.0123691521062996,null,3.0994122502343102,2.1486771367024899]
["ECS","Quantités d'énergie finale importées pour l'ECS (kWh/m2SREF)","Gaz",null,6.92472671832338,6.9773965403111804,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Bois",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,9.2784102438830391,9.2905597809210807]
[null,null,"Reseau",null,0,0,1.3960196816041399,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Elec importée",null,1.3616708002284901,1.37686837374203,0,8.2852503023563795,8.2836952299749704,8.28226101998332,8.2763845865829797,8.2755973452420406,8.2750294978066101,8.2628749380527999,8.2627773769471506,8.2633394174600792,9.4427776396399494,9.4767650443482196,9.4968762973203198,9.4622294711869603,9.4927685085758604,9.4976109844922405,null,9.4928689041858192,null,0,0]
[null,"Quantités d'énergie finale importées pour l'éclairage (kWh/m2SREF)",null,null,1.7647772017368299,1.7647848489918001,1.76487953755161,1.7647772017368299,1.7647848489918001,1.76487953755161,1.7647772017368299,1.7647848489918001,1.76487953755161,1.7647772017368299,1.7647848489918001,1.76487953755161,1.7647772017368299,1.7647848489918001,1.76487953755161,1.76483467486381,1.76487954980204,1.7656604105518401,null,1.76486626841473,null,1.7647848489918001,1.76773200650083]
[null,"Quantités d'énergie finale importées pour la ventilation (kWh/m2SREF)",null,null,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,2.8397104003871201,2.8397104003871201,2.8397104003871201,null,2.8397104003871201,null,0.691954749461415,0.691954749461415]
[null,"Quantités d'énergie finale importées pour la distribution (kWh/m2SREF)",null,null,0.659902139980724,0.60035168453650301,0.50664050271342698,0.659902139980724,0.60035168453650301,0.50664050271342698,0,0,0,0,0,0,0.71322057101799097,0.63866709385332698,0.55949730231314299,0.66267192860603696,0.58742600428504499,0.49371482246196902,null,0.58742600428504499,null,0.85494142234648496,0.80808583143494706]
[null,"Quantités d'énergie finale importées pour le déplacement des occupants (kWh/m2SREF)",null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
[null,"Production d'électricité en énergie finale par les installations photovoltaïques (kWh/m2SREF)","Elec produite",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Elec autoconsommée"]
[null,"Quantité d'énergie anuelles importées par poste en énergie finale (kWh/m2SREF par an)","Chauffage",null,37.551950007623901,30.0687694045927,21.9104964383062,37.3063360913265,29.830962834908501,21.652427824828202,22.941149565125599,18.498728927222199,13.761664153521,56.347077896565402,45.531601090806703,33.177479231040799,11.8590181492543,9.5707670554138602,7.1038867846201903,12.881689827333499,10.6441500384754,8.1037251783052699,null,10.644124139466401,null,9.5707670556135405,9.5841540028584902]
[null,null,"Refroidissement",null,3.4256072178391102,3.7884471427867101,4.0252527142654602,3.4256072178391102,3.7884471427867101,4.0252527142654602,3.4256072178391102,3.7884471427867101,4.0252527142654602,3.4256072178391102,3.7884471427867101,4.0252527142654504,3.4256072178391102,3.7884471427867101,4.0252527142650001,3.8185085964528702,4.1331200548169198,4.5348313846518398,null,4.0123691521062996,null,3.0994122502343102,2.1486771367024899]
[null,null,"ECS",null,8.2863975185518708,8.3542649140532106,8.4526560049875901,8.2852503023563795,8.2836952299749704,8.28226101998332,8.2763845865829797,8.2755973452420406,8.2750294978066101,8.2628749380527999,8.2627773769471506,8.2633394174600792,9.4427776396399494,9.4767650443482196,9.4968762973203198,9.4622294711869603,9.4927685085758604,9.4976109844922405,null,9.4928689041858192,null,9.2784102438830391,9.2905597809210807]
[null,null,"Eclairage",null,1.7647772017368299,1.7647848489918001,1.76487953755161,1.7647772017368299,1.7647848489918001,1.76487953755161,1.7647772017368299,1.7647848489918001,1.76487953755161,1.7647772017368299,1.7647848489918001,1.76487953755161,1.7647772017368299,1.7647848489918001,1.76487953755161,1.76483467486381,1.76487954980204,1.7656604105518401,null,1.76486626841473,null,1.7647848489918001,1.76773200650083]
[null,null,"Aux. ventilation",null,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,2.8397104003871201,2.8397104003871201,2.8397104003871201,null,2.8397104003871201,null,0.691954749461415,0.691954749461415]
[null,null,"Aux. distribution",null,0.659902139980724,0.60035168453650301,0.50664050271342698,0.659902139980724,0.60035168453650301,0.50664050271342698,0,0,0,0,0,0,0.71322057101799097,0.63866709385332698,0.55949730231314299,0.66267192860603696,0.58742600428504499,0.49371482246196902,null,0.58742600428504499,null,0.85494142234648496,0.80808583143494706]
[null,null," Deplacement",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Total",null,52.380588835193798,45.2685727444224,37.351879947285703,52.133827702700998,44.960196490659897,36.923416348803499,37.0998733207459,33.019513013704099,28.5187806526061,70.492292003655606,60.0395652089938,47.922905649779302,27.8973555289496,25.9313859348553,23.6423473855317,31.429644898830301,29.462054556342402,27.2352531808503,null,29.3413648688454,null,25.260270570533599,24.291163507882001]
[null,"Quantité d'énergie anuelles importées par type d'énergie en énergie finale (kWh/m2SREF par an)","Gaz",null,44.241337334573302,36.835999720216797,28.785919364352502,37.070011853289401,29.619853197573899,21.4703369064556,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Bois",null,0,0,0,0,0,0,0,0,0,43.145057035645699,34.863627348932397,25.404054427629099,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Electricité",null,8.13925150062048,8.4325730242056203,8.5659605829324192,15.063815849411601,15.340343293086001,15.453079442347899,37.0998733207459,33.019513013704099,28.5187806526061,27.3472349680099,25.175937860061399,22.5188512221502,27.8973555289496,25.9313859348553,23.6423473855317,31.429644898830301,29.462054556342402,27.2352531808503,null,29.3413648688454,null,0,0]
[null,null,"Réseau de chaleur",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
["Th-B","Bbio chaud (KWh/m2SREF)",null,null,39.5986335634827,31.851677043686301,22.493121945262299,39.5986335634827,31.851677043686301,22.493121945262299,39.5986335634827,31.851677043686301,22.493121945262299,39.5986335634827,31.851677043686301,22.493121945262299,39.5986335634827,31.851677043686301,22.493121945262299,39.5986335634827,31.851677043686301,22.493121945262299,39.5986335634827,31.851677043686301,22.493121945262299,31.851677043686301,31.851677043686301]
[null,"Bbio froid (KWh/m2SREF)",null,null,7.0978850834118701,8.6322616246525605,9.8297348986989395,7.0978850834118701,8.6322616246525605,9.8297348986989395,7.0978850834118701,8.6322616246525605,9.8297348986989395,7.0978850834118701,8.6322616246525605,9.8297348986989395,7.0978850834118701,8.6322616246525605,9.8297348986989395,7.0978850834118701,8.6322616246525605,9.8297348986989395,7.0978850834118701,8.6322616246525605,9.8297348986989395,8.6322616246525605,8.6322616246525605]
[null,"Bbio éclairage (KWh/m2SREF)",null,null,1.7663786522487901,1.7677885162952001,1.7689937975346199,1.7663786522487901,1.7677885162952001,1.7689937975346199,1.7663786522487901,1.7677885162952001,1.7689937975346199,1.7663786522487901,1.7677885162952001,1.7689937975346199,1.7663786522487901,1.7677885162952001,1.7689937975346199,1.7663786522487901,1.7677885162952001,1.7689937975346199,1.7663786522487901,1.7677885162952001,1.7689937975346199,1.7677885162952001,1.7677885162952001]
[null,"Bbio (points)",null,null,102.224930555033,89.806819918153707,73.490682675595593,102.224930555033,89.806819918153707,73.490682675595593,102.224930555033,89.806819918153707,73.490682675595593,102.224930555033,89.806819918153707,73.490682675595593,102.224930555033,89.806819918153707,73.490682675595593,102.224930555033,89.806819918153707,73.490682675595593,102.224930555033,89.806819918153707,73.490682675595593,89.806819918153707,89.806819918153707]
["Th-DB",null," Degrés-heures d'inconfort  (°C.h)",null,1096.2219643887399,1106.8930587504799,1095.03549580499,1096.2219643887399,1106.8930587504799,1095.03549580499,1096.2219643887399,1106.8930587504799,1095.03549580499,1096.2219643887399,1106.8930587504799,1095.03549580499,1096.2219643887399,1106.8930587504799,1095.03549580499,1096.2219643887399,1106.8930587504799,1095.03549580499,null,1106.8930587504799,null,1106.8930587504799,1106.8930587504799]
[null,null," Nombre d'heures d'inconfort total (h)",null,302,301,303,302,301,303,302,301,303,302,301,303,302,301,303,302,301,303,null,301,null,301,301]
[null,null,"Nombre d'heures d'inconfort d'au moins +1°C (h)",null,250,251,254,250,251,254,250,251,254,250,251,254,250,251,254,250,251,254,null,251,null,251,251]
[null,null,"Nombre d'heures d'inconfort d'au moins +2°C (h)",null,207,208,209,207,208,209,207,208,209,207,208,209,207,208,209,207,208,209,null,208,null,208,208]
["Th-DC",null," Degrés-heures d'inconfort  (°C.h)",null,1100.0156034056999,1115.2545977462601,1102.61765180115,1100.0156034056999,1115.2545977462601,1102.61765180115,1100.0156930867699,1115.25455036569,1102.61765180114,1100.01573007346,1115.25453240722,933.70993907458296,1100.01569119692,1115.25452469178,1102.6176513809501,1116.87812670938,1135.51797953954,1127.8681051846199,null,1082.85608297986]
[null,null," Nombre d'heures d'inconfort total (h)",null,302,302,303,302,302,303,302,302,303,302,302,321,302,302,303,302,306,308,null,302]
[null,null,"Nombre d'heures d'inconfort d'au moins +1°C (h)",null,251,253,253,251,253,253,251,253,253,251,253,251,251,253,253,255,257,260,null,248]
[null,null,"Nombre d'heures d'inconfort d'au moins +2°C (h)",null,208,210,210,208,210,210,208,210,210,208,210,193,208,210,210,209,211,211,null,208]
[]
[]
[null,null,null,null,"Gaz + CESI",null,null,"Gaz + CET",null,null,"PAC air/air + EJ +CET",null,null,"Bois + EJ + CET",null,null,"PAC DS air/eau ",null,null,"PAC DS air/eau + DF",null,null,"PAC DS air/eau + DF avec bypass",null,null,"PAC TS air/eau"]
["H2b",null,null,null,"V1",null,null,"V3",null,null,"V4_ssPV",null,null,"V5",null,null,"V6",null,null,"V7_DF",null,null,"V7_DF_BP",null,null,"V8 (EER=3.5 / Vt=-1.8K)","V8bis (EER=3 / Vt=0K)"]
[null,null,"Résultats - ENERGIE",null,"V1_Bbio_H2b","V1_Bbio20_H2b","V1_Bbio40_H2b","V3_Bbio_H2b","V3_Bbio20_H2b","V3_Bbio40_H2b","V4_Bbio_H2b_H2b","V4_Bbio20_H2b","V4_Bbio40_H2b","V5_Bbio_H2b","V5_Bbio20_H2b","V5_Bbio40_H2b","V6_Bbio_H2b","V6_Bbio20_H2b","V6_Bbio40_H2b","V7DF_Bbio_H2b","V7DF_Bbio20_H2b","V7DF_Bbio40_H2b","V7DFBP_Bbio_H2b","V7DFBP_Bbio20_H2b","V7DFBP_Bbio40_H2b","V8_Bbio20_H2b","V8bis_Bbio20_H2b"]
[null,"Cep (kWh/m2.an) H2b",null,null,61.297018719571703,54.765654676693302,47.302397285219598,69.640401516061303,62.990371055097498,55.390770918821801,81.256056874032794,72.630940669089597,62.350285211870599,102.449325504086,89.023133399623504,74.554090750849596,62.1470416267979,57.980382549802997,52.915461444839501,68.619083301246505,64.833766244739294,59.648546853262602,null,64.540536685236106,null,56.408060379527498,53.707449509943501]
[null,"Cep_nr (kWh/m2SREF par an)",null,null,61.297018719571703,54.765654676693302,47.302397285219598,69.640401516061303,62.990371055097498,55.390770918821801,81.256056874032794,72.630940669089597,62.350285211870599,62.435750484003599,57.305794284982099,51.667776900574196,62.1470416267979,57.980382549802997,52.915461444839501,68.619083301246505,64.833766244739294,59.648546853262602,null,64.540536685236106,null,56.408060379527498,53.707449509943501]
[null,"RCR (%)",null,null,0.13583021590637601,0.14199583271989,0.16077473191707001,9.8788911017748296E-2,0.10148080910492201,0.10562890220931399,0.14299638102582701,0.13730601482919499,0.12978859733387599,0.402496920085612,0.37639601305877601,0.34016953774339898,0.270384361640024,0.23764531976297701,0.1917639626862,0.42200902441063998,0.414090519956477,0.40517814364088001,null,0.410153791834798,null,0.14200434845174101,0.180110845092748]
["CH","Quantités d'énergie finale importées pour le chauffage (kWh/m2SREF)","Gaz",null,33.5819101176969,26.423376392471901,0,33.326031446612099,26.206721681125099,18.2945554635048,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Bois",null,0,0,0,0,0,0,0,0,0,40.013575020082797,31.717339114641401,22.8863138502753,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Reseau",null,0,0,0.164488281188475,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Elec importée",null,0.22475652485113101,0.19118700799910501,0,0.22566412469654001,0.192029056584229,0.165291579358401,20.412880864453399,16.355633634024102,11.63532983004,12.243813971521,9.7052362753492307,7.0030175793083904,10.2443636312015,8.1565950357030008,5.7570168399474797,10.623981680767599,8.6531391306964807,6.1170502162318501,null,8.65255948744921,null,8.2292550209320598,8.2122325825702909]
["FR","Quantités d'énergie finale importées pour le refroidissement (kWh/m2SREF)","Gaz",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Reseau",null,0,0,5.1399064469069202,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Elec importée",null,4.5824423217018104,4.8888313287497702,0,4.5824423217018104,4.8888313287497702,5.1399064469069202,4.5824423217015102,4.8888311579890003,5.1399115412162404,4.5824423217053898,4.88882807624777,5.1395939224718701,4.5824423217014196,4.8888307586857396,5.1399015290452699,4.9048968908254098,5.2631329249663601,5.6148272488472397,null,5.13650760362495,null,4.0975087224404696,2.9877227488240599]
["ECS","Quantités d'énergie finale importées pour l'ECS (kWh/m2SREF)","Gaz",null,6.2843296083108502,6.3833042464826404,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Bois",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,8.8434483170419806,8.8566252696308201]
[null,null,"Reseau",null,0,0,1.45776449404737,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Elec importée",null,1.41754266032794,1.4420929781970999,0,7.8877616152152399,7.8867619453657802,7.8845494130306699,7.8795374288294102,7.8795128194650603,7.8785569592494804,7.8658624130495598,7.8668061363561899,7.8666179977270296,9.0466475597991494,9.0894653656625692,9.1250605969083995,9.0553886695773809,9.0920782566646707,9.1331292147427092,null,9.0918448114409003,null,0,0]
[null,"Quantités d'énergie finale importées pour l'éclairage (kWh/m2SREF)",null,null,1.7619050155685601,1.7627374951863299,1.7630665773679099,1.7619050155685601,1.7627374951863299,1.7630665773679099,1.7619050155685601,1.7627374951863299,1.7630665773679099,1.7619050155685601,1.7627374951863299,1.7630665773679099,1.7619050155685601,1.7627374951863299,1.7630665773679099,1.76273749557708,1.7630323783595701,1.7634167893485699,null,1.7629796753445199,null,1.76289553017029,1.7646685946796199]
[null,"Quantités d'énergie finale importées pour la ventilation (kWh/m2SREF)",null,null,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,2.8397104003871201,2.8397104003871201,2.8397104003871201,null,2.8397104003871201,null,0.691954749461415,0.691954749461415]
[null,"Quantités d'énergie finale importées pour la distribution (kWh/m2SREF)",null,null,0.63912872529088005,0.57057645681439295,0.48402056227337498,0.63912872529088005,0.57057645681439295,0.48402056227337498,0,0,0,0,0,0,0.69313960348447501,0.61927857347613902,0.52972207459103204,0.64766890688559298,0.57750092837767497,0.46601693620884299,null,0.57750092837767497,null,0.90018130322659096,0.837861059157058]
[null,"Quantités d'énergie finale importées pour le déplacement des occupants (kWh/m2SREF)",null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
[null,"Production d'électricité en énergie finale par les installations photovoltaïques (kWh/m2SREF)","Elec produite",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Elec autoconsommée"]
[null,"Quantité d'énergie anuelles importées par poste en énergie finale (kWh/m2SREF par an)","Chauffage",null,33.806666642548102,26.614563400470999,18.700618808987599,33.551695571308699,26.398750737709399,18.459847042863199,20.412880864453399,16.355633634024102,11.63532983004,52.257388991603797,41.422575389990598,29.889331429583699,10.2443636312015,8.1565950357030008,5.7570168399474797,10.623981680767599,8.6531391306964807,6.1170502162318501,null,8.65255948744921,null,8.2292550209320598,8.2122325825702909]
[null,null,"Refroidissement",null,4.5824423217018104,4.8888313287497702,5.1399064469069202,4.5824423217018104,4.8888313287497702,5.1399064469069202,4.5824423217015102,4.8888311579890003,5.1399115412162404,4.5824423217053898,4.88882807624777,5.1395939224718701,4.5824423217014196,4.8888307586857396,5.1399015290452699,4.9048968908254098,5.2631329249663601,5.6148272488472397,null,5.13650760362495,null,4.0975087224404696,2.9877227488240599]
[null,null,"ECS",null,7.7018722686387902,7.8253972246797403,7.9112686956032201,7.8877616152152399,7.8867619453657802,7.8845494130306699,7.8795374288294102,7.8795128194650603,7.8785569592494804,7.8658624130495598,7.8668061363561899,7.8666179977270296,9.0466475597991494,9.0894653656625692,9.1250605969083995,9.0553886695773809,9.0920782566646707,9.1331292147427092,null,9.0918448114409003,null,8.8434483170419806,8.8566252696308201]
[null,null,"Eclairage",null,1.7619050155685601,1.7627374951863299,1.7630665773679099,1.7619050155685601,1.7627374951863299,1.7630665773679099,1.7619050155685601,1.7627374951863299,1.7630665773679099,1.7619050155685601,1.7627374951863299,1.7630665773679099,1.7619050155685601,1.7627374951863299,1.7630665773679099,1.76273749557708,1.7630323783595701,1.7634167893485699,null,1.7629796753445199,null,1.76289553017029,1.7646685946796199]
[null,null,"Aux. ventilation",null,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,2.8397104003871201,2.8397104003871201,2.8397104003871201,null,2.8397104003871201,null,0.691954749461415,0.691954749461415]
[null,null,"Aux. distribution",null,0.63912872529088005,0.57057645681439295,0.48402056227337498,0.63912872529088005,0.57057645681439295,0.48402056227337498,0,0,0,0,0,0,0.69313960348447501,0.61927857347613902,0.52972207459103204,0.64766890688559298,0.57750092837767497,0.46601693620884299,null,0.57750092837767497,null,0.90018130322659096,0.837861059157058]
[null,null," Deplacement",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Total",null,49.183969723209501,42.354060655362701,34.690835840600499,49.1148879985466,42.199612713287003,34.423344791903503,35.328720380014303,31.578669856125899,27.108819657335001,67.159553491388706,56.632901847242302,45.350564676611903,27.020452881216499,25.2088619781752,23.006722367321501,29.834384044020201,28.188594019451902,25.934150805766301,null,28.061102906624399,null,24.525243643273999,23.351065004324301]
[null,"Quantité d'énergie anuelles importées par type d'énergie en énergie finale (kWh/m2SREF par an)","Gaz",null,39.866239726007798,32.806680638954603,24.9896347293551,33.326031446612099,26.206721681125099,18.2945554635048,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Bois",null,0,0,0,0,0,0,0,0,0,40.013575020082797,31.717339114641401,22.8863138502753,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Electricité",null,9.3177299972017202,9.5473800164081197,9.7012011112447194,15.7888565519344,15.9928910321619,16.1287893283987,35.328720380014303,31.578669856125899,27.108819657335001,27.145978471305899,24.9155627326009,22.464250826336599,27.020452881216499,25.2088619781752,23.006722367321501,29.834384044020201,28.188594019451902,25.934150805766301,null,28.061102906624399,null,0,0]
[null,null,"Réseau de chaleur",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
["Th-B","Bbio chaud (KWh/m2SREF)",null,null,35.483478051730003,28.286379893661501,19.226311417569399,35.483478051730003,28.286379893661501,19.226311417569399,35.483478051730003,28.286379893661501,19.226311417569399,35.483478051730003,28.286379893661501,19.226311417569399,35.483478051730003,28.286379893661501,19.226311417569399,35.483478051730003,28.286379893661501,19.226311417569399,null,31.851677043686301,null,28.286379893661501,28.286379893661501]
[null,"Bbio froid (KWh/m2SREF)",null,null,10.328066678268,12.060328368172,13.6512251351327,10.328066678268,12.060328368172,13.6512251351327,10.328066678268,12.060328368172,13.6512251351327,10.328066678268,12.060328368172,13.6512251351327,10.328066678268,12.060328368172,13.6512251351327,10.328066678268,12.060328368172,13.6512251351327,null,8.6322616246525605,null,12.060328368172,12.060328368172]
[null,"Bbio éclairage (KWh/m2SREF)",null,null,1.7637305956376801,1.7640028313855201,1.76607236049738,1.7637305956376801,1.7640028313855201,1.76607236049738,1.7637305956376801,1.7640028313855201,1.76607236049738,1.7637305956376801,1.7640028313855201,1.76607236049738,1.7637305956376801,1.7640028313855201,1.76607236049738,1.7637305956376801,1.7640028313855201,1.76607236049738,null,1.7677885162952001,null,1.7640028313855201,1.7640028313855201]
[null,"Bbio (points)",null,null,100.441742438185,89.513430680594695,74.585434907890999,100.441742438185,89.513430680594695,74.585434907890999,100.441742438185,89.513430680594695,74.585434907890999,100.441742438185,89.513430680594695,74.585434907890999,100.441742438185,89.513430680594695,74.585434907890999,100.441742438185,89.513430680594695,74.585434907890999,null,89.806819918153707,null,89.513430680594695,89.513430680594695]
["Th-DB",null," Degrés-heures d'inconfort  (°C.h)",null,955.55452578632003,959.50290711211699,927.03435103267896,955.55452578632003,959.50290711211699,927.03435103267896,955.55452578632003,959.50290711211699,927.03435103267896,955.55452578632003,959.50290711211699,927.03435103267896,955.55452578632003,959.50290711211699,927.03435103267896,955.55452578632003,959.50290711211699,927.03435103267896,null,959.50290711211699,null,959.50290711211699,959.50290711211699]
[null,null," Nombre d'heures d'inconfort total (h)",null,322,323,321,322,323,321,322,323,321,322,323,321,322,323,321,322,323,321,null,323,null,323,323]
[null,null,"Nombre d'heures d'inconfort d'au moins +1°C (h)",null,251,253,251,251,253,251,251,253,251,251,253,251,251,253,251,251,253,251,null,253,null,253,253]
[null,null,"Nombre d'heures d'inconfort d'au moins +2°C (h)",null,193,195,192,193,195,192,193,195,192,193,195,192,193,195,192,193,195,192,null,195,null,195,195]
["Th-DC",null," Degrés-heures d'inconfort  (°C.h)",null,960.82408198097698,966.31464684540401,933.876902716107,960.82408198097698,966.31464684540401,933.876902716107,960.82408832780595,966.31477369296204,933.87689083787495,960.82400468802905,966.31706951914305,933.70993907458296,960.82409035567196,966.31507042134001,933.87691822481497,968.478716714499,976.50786184829201,944.06415721048802,null,940.56523507493705]
[null,null," Nombre d'heures d'inconfort total (h)",null,323,324,321,323,324,321,323,324,321,323,324,321,323,324,321,324,329,324,null,323]
[null,null,"Nombre d'heures d'inconfort d'au moins +1°C (h)",null,253,255,251,253,255,251,253,255,251,253,255,251,253,255,251,256,259,253,null,254]
[null,null,"Nombre d'heures d'inconfort d'au moins +2°C (h)",null,194,196,193,194,196,193,194,196,193,194,196,193,194,196,193,196,198,193,null,193]
[null,"Eges Energie (kgCO2/m²)",null,null,{"$f":"MI!E81*'CO2'!$C$6+MI!E82*'CO2'!$C$7+MI!E59*'CO2'!$C$11+MI!E62*'CO2'!$C$12+MI!E76*'CO2'!$C$14+MI!E66*'CO2'!$C$13+SUM(MI!E68:E69)*'CO2'!$C$16","v":9.6595695532356203},{"$f":"MI!F81*'CO2'!$C$6+MI!F82*'CO2'!$C$7+MI!F59*'CO2'!$C$11+MI!F62*'CO2'!$C$12+MI!F76*'CO2'!$C$14+MI!F66*'CO2'!$C$13+SUM(MI!F68:F69)*'CO2'!$C$16","v":8.0712724116669303},{"$f":"MI!G81*'CO2'!$C$6+MI!G82*'CO2'!$C$7+MI!G59*'CO2'!$C$11+MI!G62*'CO2'!$C$12+MI!G76*'CO2'!$C$14+MI!G66*'CO2'!$C$13+SUM(MI!G68:G69)*'CO2'!$C$16","v":5.8695610973530199},{"$f":"MI!H81*'CO2'!$C$6+MI!H82*'CO2'!$C$7+MI!H59*'CO2'!$C$11+MI!H62*'CO2'!$C$12+MI!H76*'CO2'!$C$14+MI!H66*'CO2'!$C$13+SUM(MI!H68:H69)*'CO2'!$C$16","v":8.5955782062682573},{"$f":"MI!I81*'CO2'!$C$6+MI!I82*'CO2'!$C$7+MI!I59*'CO2'!$C$11+MI!I62*'CO2'!$C$12+MI!I76*'CO2'!$C$14+MI!I66*'CO2'!$C$13+SUM(MI!I68:I69)*'CO2'!$C$16","v":6.992051732943823},{"$f":"MI!J81*'CO2'!$C$6+MI!J82*'CO2'!$C$7+MI!J59*'CO2'!$C$11+MI!J62*'CO2'!$C$12+MI!J76*'CO2'!$C$14+MI!J66*'CO2'!$C$13+SUM(MI!J68:J69)*'CO2'!$C$16","v":5.2042858632233511},{"$f":"MI!K81*'CO2'!$C$6+MI!K82*'CO2'!$C$7+MI!K59*'CO2'!$C$11+MI!K62*'CO2'!$C$12+MI!K76*'CO2'!$C$14+MI!K66*'CO2'!$C$13+SUM(MI!K68:K69)*'CO2'!$C$16","v":2.5839203797943884},{"$f":"MI!L81*'CO2'!$C$6+MI!L82*'CO2'!$C$7+MI!L59*'CO2'!$C$11+MI!L62*'CO2'!$C$12+MI!L76*'CO2'!$C$14+MI!L66*'CO2'!$C$13+SUM(MI!L68:L69)*'CO2'!$C$16","v":2.2830625755978167},{"$f":"MI!M81*'CO2'!$C$6+MI!M82*'CO2'!$C$7+MI!M59*'CO2'!$C$11+MI!M62*'CO2'!$C$12+MI!M76*'CO2'!$C$14+MI!M66*'CO2'!$C$13+SUM(MI!M68:M69)*'CO2'!$C$16","v":1.926188295366132},{"$f":"MI!N81*'CO2'!$C$6+MI!N82*'CO2'!$C$7+MI!N59*'CO2'!$C$11+MI!N62*'CO2'!$C$12+MI!N76*'CO2'!$C$14+MI!N66*'CO2'!$C$13+SUM(MI!N68:N69)*'CO2'!$C$16","v":3.1380824698297709},{"$f":"MI!O81*'CO2'!$C$6+MI!O82*'CO2'!$C$7+MI!O59*'CO2'!$C$11+MI!O62*'CO2'!$C$12+MI!O76*'CO2'!$C$14+MI!O66*'CO2'!$C$13+SUM(MI!O68:O69)*'CO2'!$C$16","v":2.7083752260682283},{"$f":"MI!P81*'CO2'!$C$6+MI!P82*'CO2'!$C$7+MI!P59*'CO2'!$C$11+MI!P62*'CO2'!$C$12+MI!P76*'CO2'!$C$14+MI!P66*'CO2'!$C$13+SUM(MI!P68:P69)*'CO2'!$C$16","v":2.246028682967995},{"$f":"MI!Q81*'CO2'!$C$6+MI!Q82*'CO2'!$C$7+MI!Q59*'CO2'!$C$11+MI!Q62*'CO2'!$C$12+MI!Q76*'CO2'!$C$14+MI!Q66*'CO2'!$C$13+SUM(MI!Q68:Q69)*'CO2'!$C$16","v":1.9008306115035221},{"$f":"MI!R81*'CO2'!$C$6+MI!R82*'CO2'!$C$7+MI!R59*'CO2'!$C$11+MI!R62*'CO2'!$C$12+MI!R76*'CO2'!$C$14+MI!R66*'CO2'!$C$13+SUM(MI!R68:R69)*'CO2'!$C$16","v":1.7536192449803516},{"$f":"MI!S81*'CO2'!$C$6+MI!S82*'CO2'!$C$7+MI!S59*'CO2'!$C$11+MI!S62*'CO2'!$C$12+MI!S76*'CO2'!$C$14+MI!S66*'CO2'!$C$13+SUM(MI!S68:S69)*'CO2'!$C$16","v":1.5767258775915365},{"$f":"MI!T81*'CO2'!$C$6+MI!T82*'CO2'!$C$7+MI!T59*'CO2'!$C$11+MI!T62*'CO2'!$C$12+MI!T76*'CO2'!$C$14+MI!T66*'CO2'!$C$13+SUM(MI!T68:T69)*'CO2'!$C$16","v":2.0866293801762685},{"$f":"MI!U81*'CO2'!$C$6+MI!U82*'CO2'!$C$7+MI!U59*'CO2'!$C$11+MI!U62*'CO2'!$C$12+MI!U76*'CO2'!$C$14+MI!U66*'CO2'!$C$13+SUM(MI!U68:U69)*'CO2'!$C$16","v":1.9517743443538298},{"$f":"MI!V81*'CO2'!$C$6+MI!V82*'CO2'!$C$7+MI!V59*'CO2'!$C$11+MI!V62*'CO2'!$C$12+MI!V76*'CO2'!$C$14+MI!V66*'CO2'!$C$13+SUM(MI!V68:V69)*'CO2'!$C$16","v":1.7694916179740086},{"$f":"MI!W81*'CO2'!$C$6+MI!W82*'CO2'!$C$7+MI!W59*'CO2'!$C$11+MI!W62*'CO2'!$C$12+MI!W76*'CO2'!$C$14+MI!W66*'CO2'!$C$13+SUM(MI!W68:W69)*'CO2'!$C$16","v":0},{"$f":"MI!X81*'CO2'!$C$6+MI!X82*'CO2'!$C$7+MI!X59*'CO2'!$C$11+MI!X62*'CO2'!$C$12+MI!X76*'CO2'!$C$14+MI!X66*'CO2'!$C$13+SUM(MI!X68:X69)*'CO2'!$C$16","v":1.9436057215238616},{"$f":"MI!Y81*'CO2'!$C$6+MI!Y82*'CO2'!$C$7+MI!Y59*'CO2'!$C$11+MI!Y62*'CO2'!$C$12+MI!Y76*'CO2'!$C$14+MI!Y66*'CO2'!$C$13+SUM(MI!Y68:Y69)*'CO2'!$C$16","v":0},{"$f":"MI!Z81*'CO2'!$C$6+MI!Z82*'CO2'!$C$7+MI!Z59*'CO2'!$C$11+MI!Z62*'CO2'!$C$12+MI!Z76*'CO2'!$C$14+MI!Z66*'CO2'!$C$13+SUM(MI!Z68:Z69)*'CO2'!$C$16","v":1.1358882038436051},{"$f":"MI!AA81*'CO2'!$C$6+MI!AA82*'CO2'!$C$7+MI!AA59*'CO2'!$C$11+MI!AA62*'CO2'!$C$12+MI!AA76*'CO2'!$C$14+MI!AA66*'CO2'!$C$13+SUM(MI!AA68:AA69)*'CO2'!$C$16","v":1.0596509747322689}]
[null,"Eges Energie (kgCO2/m²)","Option 1",null,7,7,7,7,7,7,7,7,7,7,7,7,7,7,7,7,7,7,7,7,7,7,7]
[null,null,"Option 2",null,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8]
[null,null,"Option 3",null,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
[]
[null,null,"Option 1 Cep",null,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90]
[null,null,"Option 1 BBIO",null,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80]
[null,null,"Option 2 Cep",null,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80]
[null,null,"Option 2 BBIO",null,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90]
[null,null,"Option 3 Cep",null,70,70,70,70,70,70,70,70,70,70,70,70,70,70,70,70,70,70,70,70,70,70,70]
[null,null,"Option 3 BBIO",null,75,75,75,75,75,75,75,75,75,75,75,75,75,75,75,75,75,75,75,75,75,75,75]
[]
[]
[null,null,null,null,"Gaz + CESI",null,null,"Gaz + CET",null,null,"PAC air/air + EJ +CET",null,null,"Bois + EJ + CET",null,null,"PAC DS air/eau ",null,null,"PAC DS air/eau + DF",null,null,"PAC DS air/eau + DF avec bypass",null,null,"PAC TS air/eau"]
["H3",null,null,null,"V1",null,null,"V3",null,null,"V4_ssPV",null,null,"V5",null,null,"V6",null,null,"V7_DF",null,null,"V7_DF_BP",null,null,"V8 (EER=3.5 / Vt=-1.8K)","V8bis (EER=3 / Vt=0K)"]
[null,null,"Résultats - ENERGIE",null,"V1_Bbio_H3","V1_Bbio20_H3","V1_Bbio40_H3","V3_Bbio_H3","V3_Bbio20_H3","V3_Bbio40_H3","V4_Bbio_H3_H3","V4_Bbio20_H3","V4_Bbio40_H3","V5_Bbio_H3","V5_Bbio20_H3","V5_Bbio40_H3","V6_Bbio_H3","V6_Bbio20_H3","V6_Bbio40_H3","V7DF_Bbio_H3","V7DF_Bbio20_H3","V7DF_Bbio40_H3","V7DF_Bbio_H3","V7DF_Bbio20_H3","V7DF_Bbio40_H3","V8_Bbio20_H3","V8bis_Bbio20_H3"]
[null,"Cep (kWh/m2.an) H3",null,null,55.612312728276599,51.1987345365145,44.336666847148201,64.290383116992601,59.812475021848698,52.8001928570812,72.525741686353101,66.696553021884498,58.358006040388197,88.447210194405301,79.389573801421804,66.974844901272903,61.047132621677399,58.163292820998002,53.933243198532701,65.618132618875194,62.990385189076598,58.431442619594897,null,62.564907355465998,null,56.799708486309001,52.622570002790503]
[null,"Cep_nr (kWh/m2SREF par an)",null,null,55.612312728276599,51.1987345365145,44.336666847148201,64.290383116992601,59.812475021848698,52.8001928570812,72.525741686353101,66.696553021884498,58.358006040388197,61.294072683133898,57.7841363035622,52.587833989859497,61.047132621677399,58.163292820998002,53.933243198532701,65.618132618875194,62.990385189076598,58.431442619594897,null,62.564907355465998,null,56.799708486309001,52.622570002790503]
[null,"RCR (%)",null,null,0.18229123106571701,0.19491881599359101,0.218452815879462,9.8446593623582601E-2,0.10031152797522799,0.10626533408654899,0.130614445559743,0.122948746268185,0.11338563764550399,0.33337570225143398,0.307492769264126,0.26702241216760603,0.20786425635768899,0.17768226442806501,0.13318589224248301,0.35506165165609599,0.34559398166005001,0.32963684517122299,null,0.34030524248654598,null,0,0]
["CH","Quantités d'énergie finale importées pour le chauffage (kWh/m2SREF)","Gaz",null,21.044729419951601,16.3680342962843,0,20.719263337662301,15.9984260910059,9.4446691614584903,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Bois",null,0,0,0,0,0,0,0,0,0,27.1531375112714,21.605437497859501,14.3870109114134,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Reseau",null,0,0,0.13422159060960101,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Elec importée",null,0.180852461025092,0.16897917919494099,0,0.18134232526570301,0.16946651887668901,0.13465381190859099,13.186621575369999,10.480776478277701,6.9188686890087201,8.3086293655159391,6.6110802987322899,4.40230309631613,6.6123573074976596,5.2405273742825704,3.5260838199453102,6.2262119792606203,4.9081002284240203,2.88561584045959,null,4.90831671069098,null,5.2417874569388303,5.2352028267171304]
["FR","Quantités d'énergie finale importées pour le refroidissement (kWh/m2SREF)","Gaz",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Reseau",null,0,0,9.2529805122294704,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Elec importée",null,9.1422788225206499,9.3138891814208602,0,9.1422788225206499,9.3138891814208602,9.2529805122294704,9.1422767088502308,9.3142021052203496,9.25191353628896,9.1467803428359993,9.3180723694971999,9.2681498223586107,9.1431758877532801,9.3131072163836102,9.2534135270653799,9.4173722505867907,9.6498757875100694,9.7384754323296896,null,9.4650471386549899,null,8.5202983264312397,6.8040523777808897]
["ECS","Quantités d'énergie finale importées pour l'ECS (kWh/m2SREF)","Gaz",null,3.0857016815917899,3.0891899505577398,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Bois",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Reseau",null,0,0,1.60068573168696,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Elec importée",null,1.56825250183944,1.5741553936291399,0,6.8239531387279602,6.8225978979345001,6.8213368168855704,6.8182632125283602,6.8174233853101098,6.8160586957411198,6.8084174391709196,6.8082855100038104,6.8076175456124499,7.9289105632633499,7.9373406364628698,7.95162063918659,7.9348688319724303,7.9402600263893603,8.0276026566769403,null,7.9400537942708302,null,7.6470104127135503,7.6338077496043404]
[null,"Quantités d'énergie finale importées pour l'éclairage (kWh/m2SREF)",null,null,1.6938149217696099,1.69414459559321,1.69425043401641,1.6938149217696099,1.69414459559321,1.69425043401641,1.6938149217696099,1.69414459559321,1.69425043401641,1.6938149217696099,1.69414459559321,1.69425043401641,1.6938149217696099,1.69414459559321,1.69425043401641,1.6941445960177499,1.6946446085000899,1.6952190521822901,null,1.6942418290486201,null,1.69383154862083,1.6984269926457201]
[null,"Quantités d'énergie finale importées pour la ventilation (kWh/m2SREF)",null,null,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,2.8397104003871201,2.8397104003871201,2.8397104003871201,null,2.8397104003871201,null,0.691954749461415,0.691954749461415]
[null,"Quantités d'énergie finale importées pour la distribution (kWh/m2SREF)",null,null,0.410621163702591,0.35753354838410001,0.25505136924753402,0.410621163702591,0.35753354838410001,0.25505136924753402,0,0,0,0,0,0,0.47201814489701999,0.41131361085891899,0.33191300359995801,0.41731481954709598,0.35453294404001101,0.218351669962142,null,0.35476375975878699,null,0.90064293466414302,0.81593356587333299]
[null,"Quantités d'énergie finale importées pour le déplacement des occupants (kWh/m2SREF)",null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
[null,"Production d'électricité en énergie finale par les installations photovoltaïques (kWh/m2SREF)","Elec produite",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Elec autoconsommée"]
[null,"Quantité d'énergie anuelles importées par poste en énergie finale (kWh/m2SREF par an)","Chauffage",null,21.225581880976701,16.537013475479199,9.9350710090478493,20.900605662928001,16.1678926098826,9.5793229733670806,13.186621575369999,10.480776478277701,6.9188686890087201,35.461766876787301,28.216517796591798,18.789314007729502,6.6123573074976596,5.2405273742825704,3.5260838199453102,6.2262119792606203,4.9081002284240203,2.88561584045959,null,4.90831671069098,null,5.2417874569388303,5.2352028267171304]
[null,null,"Refroidissement",null,9.1422788225206499,9.3138891814208602,9.2529805122294704,9.1422788225206499,9.3138891814208602,9.2529805122294704,9.1422767088502308,9.3142021052203496,9.25191353628896,9.1467803428359993,9.3180723694971999,9.2681498223586107,9.1431758877532801,9.3131072163836102,9.2534135270653799,9.4173722505867907,9.6498757875100694,9.7384754323296896,null,9.4650471386549899,null,8.5202983264312397,6.8040523777808897]
[null,null,"ECS",null,4.6539541834312397,4.6633453441868697,4.7894710697187497,6.8239531387279602,6.8225978979345001,6.8213368168855704,6.8182632125283602,6.8174233853101098,6.8160586957411198,6.8084174391709196,6.8082855100038104,6.8076175456124499,7.9289105632633499,7.9373406364628698,7.95162063918659,7.9348688319724303,7.9402600263893603,8.0276026566769403,null,7.9400537942708302,null,7.6470104127135503,7.6338077496043404]
[null,null,"Eclairage",null,1.6938149217696099,1.69414459559321,1.69425043401641,1.6938149217696099,1.69414459559321,1.69425043401641,1.6938149217696099,1.69414459559321,1.69425043401641,1.6938149217696099,1.69414459559321,1.69425043401641,1.6938149217696099,1.69414459559321,1.69425043401641,1.6941445960177499,1.6946446085000899,1.6952190521822901,null,1.6942418290486201,null,1.69383154862083,1.6984269926457201]
[null,null,"Aux. ventilation",null,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,0.691954749461415,2.8397104003871201,2.8397104003871201,2.8397104003871201,null,2.8397104003871201,null,0.691954749461415,0.691954749461415]
[null,null,"Aux. distribution",null,0.410621163702591,0.35753354838410001,0.25505136924753402,0.410621163702591,0.35753354838410001,0.25505136924753402,0,0,0,0,0,0,0.47201814489701999,0.41131361085891899,0.33191300359995801,0.41731481954709598,0.35453294404001101,0.218351669962142,null,0.35476375975878699,null,0.90064293466414302,0.81593356587333299]
[null,null," Deplacement",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Total",null,37.818205721862199,33.257880894525698,26.618779143721401,39.6632284591103,35.048012582676698,28.294896855207501,31.532931167979601,28.9985013138628,25.3730461045166,53.802734330025203,46.728975021147498,37.251286559178403,26.542231574642301,25.288388183042599,23.4492361732751,28.5296228777718,27.3871239952507,25.404975051997798,null,27.2021336328113,null,24.6955254288311,22.8793782620833]
[null,"Quantité d'énergie anuelles importées par type d'énergie en énergie finale (kWh/m2SREF par an)","Gaz",null,24.130431101543401,19.457224246841999,12.98963475647,20.719263337662301,15.9984260910059,9.4446691614584903,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Bois",null,0,0,0,0,0,0,0,0,0,27.1531375112714,21.605437497859501,14.3870109114134,0,0,0,0,0,0,null,0,null,0,0]
[null,null,"Electricité",null,13.6877746203188,13.8006566476837,13.629144387250401,18.943965121447899,19.049586491670802,18.850227693749002,31.532931167979601,28.9985013138628,25.3730461045166,26.649596818753899,25.123537523287901,22.864275647765002,26.542231574642301,25.288388183042599,23.4492361732751,28.5296228777718,27.3871239952507,25.404975051997798,null,27.2021336328113,null,0,0]
[null,null,"Réseau de chaleur",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,null,0,0]
["Th-B","Bbio chaud (KWh/m2SREF)",null,null,21.3744679763557,16.491560968553301,9.4473089356487208,21.3744679763557,16.491560968553301,9.4473089356487208,21.3744679763557,16.491560968553301,9.4473089356487208,21.3744679763557,16.491560968553301,9.4473089356487208,21.3744679763557,16.491560968553301,9.4473089356487208,21.3744679763557,16.491560968553301,9.4473089356487208,null,31.851677043686301,null,16.491560968553301,16.491560968553301]
[null,"Bbio froid (KWh/m2SREF)",null,null,26.999991681216599,28.255829488557598,29.164636094876698,26.999991681216599,28.255829488557598,29.164636094876698,26.999991681216599,28.255829488557598,29.164636094876698,26.999991681216599,28.255829488557598,29.164636094876698,26.999991681216599,28.255829488557598,29.164636094876698,26.999991681216599,28.255829488557598,29.164636094876698,null,8.6322616246525605,null,28.255829488557598,28.255829488557598]
[null,"Bbio éclairage (KWh/m2SREF)",null,null,1.69796658353078,1.6989250193379399,1.69932350416981,1.69796658353078,1.6989250193379399,1.69932350416981,1.69796658353078,1.6989250193379399,1.69932350416981,1.69796658353078,1.6989250193379399,1.69932350416981,1.69796658353078,1.6989250193379399,1.69932350416981,1.69796658353078,1.6989250193379399,1.69932350416981,null,1.7677885162952001,null,1.6989250193379399,1.6989250193379399]
[null,"Bbio (points)",null,null,105.238752232799,97.989406010911594,85.720507581899795,105.238752232799,97.989406010911594,85.720507581899795,105.238752232799,97.989406010911594,85.720507581899795,105.238752232799,97.989406010911594,85.720507581899795,105.238752232799,97.989406010911594,85.720507581899795,105.238752232799,97.989406010911594,85.720507581899795,null,89.806819918153707,null,97.989406010911594,97.989406010911594]
["Th-DB",null," Degrés-heures d'inconfort  (°C.h)",null,2023.4326582077999,2051.2815732959398,2013.4112123621201,2023.4326582077999,2051.2815732959398,2013.4112123621201,2023.4326582077999,2051.2815732959398,2013.4112123621201,2023.4326582077999,2051.2815732959398,2013.4112123621201,2023.4326582077999,2051.2815732959398,2013.4112123621201,2023.4326582077999,2051.2815732959398,2013.4112123621201,null,2051.2815732959398,null,2051.2815732959398,2051.2815732959398]
[null,null," Nombre d'heures d'inconfort total (h)",null,920,929,928,920,929,928,920,929,928,920,929,928,920,929,928,920,929,928,null,929,null,929,929]
[null,null,"Nombre d'heures d'inconfort d'au moins +1°C (h)",null,685,698,680,685,698,680,685,698,680,685,698,680,685,698,680,685,698,680,null,698,null,698,698]
[null,null,"Nombre d'heures d'inconfort d'au moins +2°C (h)",null,438,442,429,438,442,429,438,442,429,438,442,429,438,442,429,438,442,429,null,442,null,442,442]
["Th-DC",null," Degrés-heures d'inconfort  (°C.h)",null,2035.8970264683501,2064.1156930971802,2024.7034747492,2035.8970264683501,2064.1156930971802,2024.7034747492,2035.9003958292999,2064.1379347308998,2024.70680668357,2035.89923707714,2064.1231518290301,2024.7051920896999,2035.89641121401,2064.0945072192899,2024.70864526896,2074.08885682137,2100.7376497400201,2063.8729254222098,null,2023.54713846052]
[null,null," Nombre d'heures d'inconfort total (h)",null,920,934,931,920,934,931,920,934,931,920,934,931,920,934,931,938,948,942,null,923]
[null,null,"Nombre d'heures d'inconfort d'au moins +1°C (h)",null,689,702,686,689,702,686,689,702,686,689,702,686,689,702,686,708,715,710,null,687]
[null,null,"Nombre d'heures d'inconfort d'au moins +2°C (h)",null,438,444,431,438,444,431,438,444,431,438,444,431,438,444,431,447,455,447,null,436]

{"sheet":"Graph MI","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"LC","index":2,"n_rows":156,"n_cols":40,"rows_kept":156,"cut":false,"hidden":false,"merged":[[7,0,10,0],[11,0,13,0],[14,0,17,0],[56,0,59,0],[60,0,62,0],[63,0,66,0],[110,10,110,12],[110,13,110,15],[109,10,109,12],[109,13,109,15],[73,1,80,1],[73,2,73,3],[74,2,74,3],[75,2,75,3],[76,2,76,3],[77,2,77,3],[78,2,78,3],[79,2,79,3],[80,2,80,3],[89,0,92,0],[89,1,92,1],[89,2,89,3],[90,2,90,3],[91,2,91,3],[85,0,88,0],[36,0,39,0],[40,0,43,0],[152,0,155,0],[152,1,155,1],[152,2,152,3],[153,2,153,3],[154,2,154,3],[155,2,155,3],[44,0,47,0],[44,1,47,1],[44,2,44,3],[45,2,45,3],[46,2,46,3],[47,2,47,3],[93,0,96,0],[93,1,96,1],[93,2,93,3],[94,2,94,3],[95,2,95,3],[96,2,96,3],[148,0,151,0],[148,1,151,1],[148,2,148,3],[149,2,149,3],[150,2,150,3],[151,2,151,3],[140,1,143,1],[140,2,140,3],[141,2,141,3],[142,2,142,3],[143,2,143,3],[144,0,147,0],[144,1,144,3],[145,1,145,3],[146,1,146,3],[147,1,147,3],[132,1,139,1],[132,2,132,3],[133,2,133,3],[134,2,134,3],[135,2,135,3],[136,2,136,3],[137,2,137,3],[138,2,138,3],[139,2,139,3],[115,0,118,0],[119,1,121,1],[119,2,119,3],[120,2,120,3],[121,2,121,3],[128,1,128,3],[129,1,129,3],[130,1,131,1],[130,2,130,3],[131,2,131,3],[122,1,125,1],[122,2,122,3],[123,2,123,3],[124,2,124,3],[125,2,125,3],[126,1,126,3],[119,0,121,0],[122,0,125,0],[110,4,110,6],[110,7,110,9],[127,1,127,3],[81,1,84,1],[81,2,81,3],[82,2,82,3],[83,2,83,3],[84,2,84,3],[85,1,85,3],[86,1,86,3],[87,1,87,3],[88,1,88,3],[109,4,109,6],[109,7,109,9],[112,1,112,3],[113,1,113,3],[114,1,114,3],[115,1,118,1],[115,2,115,3],[97,1,97,2],[92,2,92,3],[116,2,116,3],[117,2,117,3],[118,2,118,3],[69,1,69,3],[70,1,70,3],[71,1,72,1],[71,2,71,3],[72,2,72,3],[63,1,66,1],[63,2,63,3],[64,2,64,3],[65,2,65,3],[66,2,66,3],[67,1,67,3],[68,1,68,3],[51,10,51,12],[51,13,51,15],[53,1,53,3],[54,1,54,3],[55,1,55,3],[56,1,59,1],[56,2,56,3],[22,1,23,1],[22,2,22,3],[23,2,23,3],[40,1,43,1],[40,2,40,3],[41,2,41,3],[42,2,42,3],[43,2,43,3],[57,2,57,3],[58,2,58,3],[59,2,59,3],[37,1,37,3],[38,1,38,3],[39,1,39,3],[50,10,50,12],[50,13,50,15],[60,1,62,1],[60,2,60,3],[61,2,61,3],[62,2,62,3],[51,4,51,6],[51,7,51,9],[24,1,31,1],[24,2,24,3],[25,2,25,3],[26,2,26,3],[27,2,27,3],[28,2,28,3],[29,2,29,3],[30,2,30,3],[31,2,31,3],[32,1,35,1],[32,2,32,3],[33,2,33,3],[34,2,34,3],[35,2,35,3],[36,1,36,3],[50,4,50,6],[50,7,50,9],[2,10,2,12],[2,13,2,15],[4,1,4,3],[5,1,5,3],[6,1,6,3],[7,1,10,1],[7,2,7,3],[2,16,2,18],[8,2,8,3],[9,2,9,3],[10,2,10,3],[11,1,13,1],[11,2,11,3],[12,2,12,3],[13,2,13,3],[2,4,2,6],[2,7,2,9],[19,1,19,3],[20,1,20,3],[21,1,21,3],[14,1,17,1],[14,2,14,3],[15,2,15,3],[16,2,16,3],[17,2,17,3],[18,1,18,3],[2,28,2,30],[51,28,51,30],[110,28,110,30],[51,16,51,18],[110,16,110,18],[2,19,2,21],[51,19,51,21],[110,19,110,21],[2,22,2,24],[51,22,51,24],[110,22,110,24],[2,25,2,27],[51,25,51,27],[110,25,110,27],[50,16,50,18],[50,19,50,21],[50,22,50,24],[50,25,50,27],[50,28,50,30],[109,16,109,18],[109,19,109,21],[109,22,109,24],[109,25,109,27],[109,28,109,30],[1,4,1,6],[1,7,1,9],[1,10,1,12],[1,13,1,15],[1,16,1,18],[1,19,1,21],[1,22,1,24],[1,25,1,27],[1,28,1,30],[110,34,110,36],[1,37,1,39],[50,37,50,39],[109,37,109,39],[1,31,1,33],[50,34,50,36],[109,34,109,36],[1,34,1,36],[50,31,50,33],[109,31,109,33],[2,31,2,33],[2,34,2,36],[2,37,2,39],[51,31,51,33],[110,31,110,33],[51,34,51,36],[51,37,51,39],[110,37,110,39]]}
[]
[null,null,null,null,"Gaz  collectif",null,null,"Gaz collectif + CESC",null,null,"Gaz individuel",null,null,"Gaz indiv. + DF",null,null,"Gaz + CET collectif",null,null,"Bois",null,null,"PAC O/O DS",null,null,"EJ + CET air extrait",null,null,"RCU",null,null,"Gaz indiv. + CET extrait",null,null,"Gaz indiv. + CET extérieur",null,null,"PAC DS air/eau"]
["H1a",null,null,null,"V1",null,null,"V2",null,null,"V3",null,null,"V4",null,null,"V6",null,null,"V7",null,null,"V8",null,null,"V9",null,null,"V10",null,null,"V11",null,null,"V12 corrigé",null,null,"V13"]
[null,null,"Résultats - ENERGIE",null,"V1_Bbio_H1a","V1_Bbio20_H1a","V1_Bbio40_H1a","V2_Bbio_H1a","V2_Bbio20_H1a","V2_Bbio40_H1a","V3_Bbio_H1a","V3_Bbio20_H1a","V3_Bbio40_H1a","V4_Bbio_H1a","V4_Bbio20_H1a","V4_Bbio40_H1a","V6_Bbio_H1a","V6_Bbio20_H1a","V6_Bbio40_H1a","V7_Bbio_H1a","V7_Bbio20_H1a","V7_Bbio40_H1a","V8_Bbio_H1a","V8_Bbio20_H1a","V8_Bbio40_H1a","V9_Bbio_H1a","V9_Bbio20_H1a","V9_Bbio40_H1a","V10_Bbio_H1a","V10_Bbio20_H1a","V10_Bbio40_H1a","V11_Bbio_H1a","V11_Bbio20_H1a","V11_Bbio40_H1a","V12_Bbio_H1a","V12_Bbio20_H1a","V12_Bbio40_H1a","V13_Bbio_H1a","V13_Bbio20_H1a","V13_Bbio40_H1a"]
[null,"Cep (kWh/m2SREF par an)",null,null,100.271144415572,94.205173476140899,87.534579748020803,91.0317567229486,84.912645117603006,78.093237031656599,92.468313201552903,86.272524912054294,79.665583770448706,100.10411696990001,null,87.881993038962804,92.776420877913594,null,null,104.05001728202301,97.4109365662773,null,72.641580412779703,69.746377023233904,null,143.817121139215,null,111.477207413532,116.917958202637,109.01393649116601,null,97.090548855764695,null,null,101.33325786564301,94.796010116478001,88.046834899352305,80.298196802601396]
[null,"Cep_nr (kWh/m2SREF par an)",null,null,100.271144415572,94.205173476140899,87.534579748020803,91.0317567229486,84.912645117603006,78.093237031656599,92.468313201552903,86.272524912054294,79.665583770448706,100.10411696990001,null,87.881993038962804,92.776420877913594,null,null,32.0424461906996,32.600765528932797,null,72.641580412779703,69.746377023233904,null,143.817121139215,null,111.477207413532,54.338271232622198,52.190242532686398,null,97.090548855764695,null,null,101.33325786564301,94.796010116478001,88.046834899352305,80.298196802601396]
[null,"RCR (%)",null,null,1.99361854865296E-2,1.6331836321712399E-2,1.19725883396681E-2,0.119470135766776,0.122887858499389,0.127769593993804,0,0,0,0.28857915709093002,null,0.32597745381924598,0.110283119036464,null,null,0.67627253713880098,0.64876267533354104,null,0.33429725721749498,0.318476253824858,null,1.5633595039954899E-3,null,2.0389196556836698E-3,0.53354799925597596,0.51934962496006598,null,1.54424170911519E-2,null,null,1.46977668767689E-2,1.01171084936055E-2,5.6614941807511003E-3,0.22555240768142901]
["CH","Quantités d'énergie finale importées pour le chauffage (kWh/m2SREF)","Gaz",null,39.351624932878103,32.800531859494399,25.601026262290802,39.424550773888598,32.843772129078999,25.5761289295436,40.552476660509399,33.946257535971,26.7553828065281,44.921250497444802,null,31.023733011938099,39.9301989392184,null,null,0,0,null,0,0,null,0,null,0,0,0,null,40.847159101041903,null,null,40.847159101041903,34.0816215885297,26.9221039336968,0]
[null,null,"Bois",null,0,0,0,0,0,0,0,0,0,0,null,0,0,null,null,40.577044741538998,33.386991627964903,null,0,0,null,0,null,0,0,0,null,0,null,null,0,0,0,0]
[null,null,"Reseau",null,0,0,0,0,0,0,0,0,0,0,null,0,0,null,null,0,0,null,10.6980430591827,0,null,0,null,0,59.894375528691597,51.644422378101702,null,0,null,null,0,0,0,0]
[null,null,"Elec importée",null,0.1327986758245,0.111422791514466,8.7566362743141599E-2,0.133932956377388,0.112442587458494,8.8353371750012899E-2,0.41090236331213897,0.39512172846365101,0.355116241377742,0.39471902343496501,null,0.338888553534338,0.13550984719008199,null,null,8.5940679492938002E-2,7.6111070860005001E-2,null,0,9.1759745921999194,null,39.519825839447201,null,24.9786781944434,0,0,null,0.441641904260346,null,null,0.441641904260346,0.400109157610752,0.36000163644878902,13.618632793743799]
["FR","Quantités d'énergie finale importées pour le refroidissement (kWh/m2SREF)","Gaz",null,0,0,0,0,0,0,0,0,0,0,null,0,0,null,null,0,0,null,0,0,null,0,null,0,0,0,null,0,null,null,0,0,0,0]
[null,null,"Reseau",null,0,0,0,0,0,0,0,0,0,0,null,0,0,null,null,0,0,null,4.1667552942995396,0,null,0,null,0,0,0,null,0,null,null,0,0,0,0]
[null,null,"Elec importée",null,4.2268716017909096,4.4763921964801696,4.74018948231409,4.1858587636460696,4.4288923662299604,4.6791810845338304,4.1165416949397802,4.3443469736773901,4.5984178942337204,4.6914865106126999,null,5.4814773676613102,4.1883441787824003,null,null,4.3631350987287698,4.6323190984812204,null,0,4.4086114378949999,null,4.3396489939852598,null,4.8685274861533001,3.65110297771013,3.8218808097012702,null,4.0162211295572403,null,null,4.0162211295572403,4.2081003096597804,4.4640563281340198,4.1592064285530004]
["ECS","Quantités d'énergie finale importées pour l'ECS (kWh/m2SREF)","Gaz",null,29.009052873600499,29.011474777928299,29.0558556002091,19.736282497702401,19.730000776762399,19.7242233282089,23.7544864814442,23.774602426995699,23.876979266184801,23.819927062752502,null,23.9399080571593,9.0134113103994498,null,null,0,0,null,0,0,null,0,null,0,0,0,null,0,null,null,0,0,0,0]
[null,null,"Bois",null,0,0,0,0,0,0,0,0,0,0,null,0,0,null,null,31.430526349784301,31.4231794093796,null,0,0,null,0,null,0,0,0,null,0,null,null,0,0,0,0]
[null,null,"Reseau",null,0,0,0,0,0,0,0,0,0,0,null,0,0,null,null,0,0,null,7.2967228021073698,0,null,0,null,0,29.505177285615598,29.532283276868998,null,0,null,null,0,0,0,0]
[null,null,"Elec importée",null,9.5157258738970393E-2,9.5234850957324799E-2,9.5796171531160601E-2,0.11688651603247099,0.117031255397634,0.117601310849809,0.333371747381071,0.34062308502878103,0.37146031477114999,0.35513172210293298,null,0.39321611991946698,5.3126490827545698,null,null,7.2694468493613495E-2,7.3811163057101906E-2,null,0,7.3368308024181799,null,11.510575774564501,null,11.461381263563799,0,0,null,12.6076753118105,null,null,14.452331403062001,14.451426638256001,14.4487429521152,7.7123910033509198]
[null,"Quantités d'énergie finale importées pour l'éclairage (kWh/m2SREF)",null,null,1.71683797332871,1.71698964541994,1.71707808263649,1.7164663060673,1.71698964541994,1.7170776251570901,1.7164663060673,1.71630920299531,1.71648161093593,1.7166354243137301,null,1.71760734781225,1.7164663060673,null,null,1.7168479723397501,1.71704952453875,null,1.71646712227785,1.71698964541994,null,1.7168471510110399,null,1.7173354532159999,1.7159881272121,1.71631084516164,null,1.7164628852296899,null,null,1.7164628852296899,1.71625156902271,1.7163960968284,1.7164663060673]
[null,"Quantités d'énergie finale importées pour la ventilation (kWh/m2SREF)",null,null,1.1596368034273401,1.1597200897323301,1.1597759151590401,1.15963101232086,1.1597198386951799,1.1597631757795901,1.1596285470166501,1.15968606363191,1.1597475676822799,1.9344332454745401,null,1.9346673974767099,1.15963101232086,null,null,1.15965345080586,1.1597341857593799,null,1.1596313563676099,1.1597190637543999,null,1.1596489648810899,null,1.1597922718678799,1.4998798094124099E-3,1.5608401930602899E-3,null,1.15962409383586,null,null,1.15962409383586,1.15964808853973,1.15972606005069,1.1596308049423401]
[null,"Quantités d'énergie finale importées pour la distribution (kWh/m2SREF)",null,null,2.2601772237692499,2.2415896278296499,2.21160886007288,2.2615113051590701,2.2426671491863099,2.2131630404661302,0.224518204469593,0.17504393525393699,0.13927985946243801,0.26101830685795602,null,0.16383377689815901,2.2625069442001999,null,null,2.2505902938040001,2.2325844593306998,null,2.2630422610432999,2.2437498274271501,null,0,null,0,2.31329671703346,2.2807549666504898,null,0.229386014633536,null,null,0.229386014633536,0.17938808633626499,0.14441053137295401,2.2632957626169801]
[null,"Quantités d'énergie finale importées pour le déplacement des occupants (kWh/m2SREF)",null,null,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,null,4.2826363801175296,4.2826363801175296,null,null,4.2826363801175296,4.2826363801175296,null,4.28263841658804,4.2826363801175296,null,4.2826363801175296,null,4.2826363801175296,4.2826363801175296,4.2826363801175296,null,4.2826363801175296,null,null,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296]
[null,"Production d'électricité en énergie finale par les installations photovoltaïques (kWh/m2SREF)","Elec produite",null,0,0,0,0,0,0,0,0,0,0,null,0,0,null,null,0,0,null,0,0,null,0,null,0,0,0,null,0,null,null,0,0,0,0]
[null,null,"Elec autoconsommée",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0]
[null,"Quantité d'énergie anuelles importées par poste en énergie finale (kWh/m2SREF par an)","Chauffage",null,39.484423608702599,32.911954651008799,25.688592625033898,39.558483730265998,32.956214716537502,25.664482301293599,40.963379023821503,34.3413792644346,27.1104990479059,45.315969520879797,null,31.362621565472399,40.0657087864085,null,null,40.662985421031898,33.463102698824898,null,10.698048146294299,9.1759745921999194,null,39.519825839447201,null,24.9786781944434,59.894375528691597,51.644422378101702,null,41.288801005302297,null,null,41.288801005302297,34.4817307461404,27.2821055701456,13.618632793743799]
[null,null,"Refroidissement",null,4.2268716017909096,4.4763921964801696,4.74018948231409,4.1858587636460696,4.4288923662299604,4.6791810845338304,4.1165416949397802,4.3443469736773901,4.5984178942337204,4.6914865106126999,null,5.4814773676613102,4.1883441787824003,null,null,4.3631350987287698,4.6323190984812204,null,4.1667572756665097,4.4086114378949999,null,4.3396489939852598,null,4.8685274861533001,3.65110297771013,3.8218808097012702,null,4.0162211295572403,null,null,4.0162211295572403,4.2081003096597804,4.4640563281340198,4.1592064285530004]
[null,null,"ECS",null,29.104210132339499,29.1067096288856,29.151651771740301,19.853169013734899,19.847032032160001,19.8418246390587,24.087858228825301,24.115225512024502,24.2484395809559,24.175058784855398,null,24.333124177078801,14.326060393154,null,null,31.503220818277899,31.496990572436701,null,7.2967262718301003,7.3368308024181799,null,11.510575774564501,null,11.461381263563799,29.505177285615598,29.532283276868998,null,12.6076753118105,null,null,14.452331403062001,14.451426638256001,14.4487429521152,7.7123910033509198]
[null,null,"Eclairage",null,1.71683797332871,1.71698964541994,1.71707808263649,1.7164663060673,1.71698964541994,1.7170776251570901,1.7164663060673,1.71630920299531,1.71648161093593,1.7166354243137301,null,1.71760734781225,1.7164663060673,null,null,1.7168479723397501,1.71704952453875,null,1.71646712227785,1.71698964541994,null,1.7168471510110399,null,1.7173354532159999,1.7159881272121,1.71631084516164,null,1.7164628852296899,null,null,1.7164628852296899,1.71625156902271,1.7163960968284,1.7164663060673]
[null,null,"Aux. ventilation",null,1.1596368034273401,1.1597200897323301,1.1597759151590401,1.15963101232086,1.1597198386951799,1.1597631757795901,1.1596285470166501,1.15968606363191,1.1597475676822799,1.9344332454745401,null,1.9346673974767099,1.15963101232086,null,null,1.15965345080586,1.1597341857593799,null,1.1596313563676099,1.1597190637543999,null,1.1596489648810899,null,1.1597922718678799,1.4998798094124099E-3,1.5608401930602899E-3,null,1.15962409383586,null,null,1.15962409383586,1.15964808853973,1.15972606005069,1.1596308049423401]
[null,null,"Aux. distribution",null,2.2601772237692499,2.2415896278296499,2.21160886007288,2.2615113051590701,2.2426671491863099,2.2131630404661302,0.224518204469593,0.17504393525393699,0.13927985946243801,0.26101830685795602,null,0.16383377689815901,2.2625069442001999,null,null,2.2505902938040001,2.2325844593306998,null,2.2630422610432999,2.2437498274271501,null,0,null,0,2.31329671703346,2.2807549666504898,null,0.229386014633536,null,null,0.229386014633536,0.17938808633626499,0.14441053137295401,2.2632957626169801]
[null,null," Deplacement",null,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,null,4.2826363801175296,4.2826363801175296,null,null,4.2826363801175296,4.2826363801175296,null,4.28263841658804,4.2826363801175296,null,4.2826363801175296,null,4.2826363801175296,4.2826363801175296,4.2826363801175296,null,4.2826363801175296,null,null,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296]
[null,null,"Total",null,82.234793723475804,75.895992219474095,68.951533117074206,73.017756511311703,66.6341521283464,59.558128246406497,76.551028385257595,70.134627332135196,63.255501941293701,82.377238173111607,null,69.275968012517197,68.0013540010508,null,null,85.939069435105793,78.984416919489206,null,31.583310850067701,30.324511749232101,null,62.529183104006698,null,48.4683510493619,101.36407689619,93.279849496794796,null,65.300806820486599,null,null,67.145462911738093,60.479181818072398,53.498073918764398,34.912259479391899]
[null,"Quantité d'énergie anuelles importées par type d'énergie en énergie finale (kWh/m2SREF par an)","Gaz",null,68.360677806478606,61.812006637422598,54.656881862499901,59.160833271591002,52.573772905841402,45.3003522577525,64.306963141953602,57.720859962966699,50.632362072712901,68.741177560197301,null,54.963641069097399,48.943610249617898,null,null,0,0,null,0,0,null,0,null,0,0,0,null,40.847159101041903,null,null,40.847159101041903,34.0816215885297,26.9221039336968,0]
[null,null,"Bois",null,0,0,0,0,0,0,0,0,0,0,null,0,0,null,null,72.0075710913233,64.810171037344503,null,0,0,null,0,null,0,0,0,null,0,null,null,0,0,0,0]
[null,null,"Electricité",null,13.8741159169972,14.083985582051399,14.294651254574299,13.8569232397207,14.060379222505,14.257775988654,12.2440652433041,12.4137673691685,12.6231398685808,13.636060612914401,null,14.3123269434198,19.057743751432898,null,null,13.931498343782501,14.174245882144699,null,31.583310850067701,30.324511749232101,null,62.529183104006698,null,48.4683510493619,11.964524081882599,12.103143841824,null,24.4536477194447,null,null,26.298303810696201,26.397560229542801,26.575969985067601,34.912259479391899]
[null,null,"Réseau de chaleur",null,0,0,0,0,0,0,0,0,0,0,null,0,0,null,null,0,0,null,0,0,null,0,null,0,89.399552814307199,81.176705654970803,null,0,null,null,0,0,0,0]
["Th-B","Bbio chaud (KWh/m2SREF)",null,null,43.209479715486196,35.9886851861705,28.112139819532999,43.209478298263598,35.9886851861705,28.112139837867701,43.209476881026703,35.988631374596501,28.112139837867701,43.209476881026703,null,28.112139837867701,43.209484251913103,null,null,43.209478298263598,35.988631374596501,null,43.209478298263598,35.988631374596501,null,43.2682299312902,null,28.112139837867701,43.209478298263598,35.988631374596501,null,43.209476881026703,null,null,43.209476881026703,null,null,43.209478298263598]
[null,"Bbio froid (KWh/m2SREF)",null,null,8.0826603168526407,8.8034940556096206,10.0956866552976,8.0826445679776207,8.8034940556096206,10.0956844619602,8.0826594001122896,8.8034881878032394,10.0956844619602,8.0826594001122896,null,10.0956844619602,8.0826464058241196,null,null,8.0826445679776207,8.8034881878032394,null,8.0826445679776207,8.8034881878032394,null,8.0770837824288595,null,10.0956844619602,8.0826445679776207,8.8034881878032394,null,8.0826594001122896,null,null,8.0826594001122896,null,null,8.0826445679776207]
[null,"Bbio éclairage (KWh/m2SREF)",null,null,0,0,0,0,0,0,0,0,0,0,null,0,0,null,null,0,0,null,0,0,null,0,null,0,0,0,null,0,null,null,0,null,null,0]
[null,"Bbio (points)",null,null,102.584280064678,89.584358483560294,76.415652949661194,102.584245732482,89.584358483560294,76.415648599655896,102.584272562278,89.584239124799495,76.415648599655896,102.584272562278,null,76.415648599655896,102.584261315474,null,null,102.584245732482,89.584239124799495,null,102.584245732482,89.584239124799495,null,102.690627427438,null,76.415648599655896,102.584245732482,89.584239124799495,null,102.584272562278,null,null,102.584272562278,null,null,102.584245732482]
["Th-DB",null," Degrés-heures d'inconfort  (°C.h)",null,506.43363774149248,487.00216138476702,471.65838610603203,503.85900602329298,486.96504093415001,471.15801227616453,503.38127385200102,486.05464477613452,470.89038884288595,503.38127385200102,null,470.89038884288595,503.32644632857102,null,null,503.85900602329298,486.96504093415001,null,503.85900602329298,486.96504093415001,null,519.30245472540355,null,482.26466483941749,503.85900602329298,486.96504093415001,null,503.38127385200102,null,null,null,null,null,503.85900602329298]
[null,null," Nombre d'heures d'inconfort total (h)",null,216,214,212.5,216,215,213,214.5,214,212,214.5,null,212,214.5,null,null,216,215,null,216,215,null,219,null,212.5,216,215,null,214.5,null,null,null,null,null,216]
[null,null,"Nombre d'heures d'inconfort d'au moins +1°C (h)",null,160.5,159.5,155.5,160.5,159,155,160,159,155,160,null,155,160.5,null,null,160.5,159,null,160.5,159,null,164.5,null,158.5,160.5,159,null,160,null,null,null,null,null,160.5]
[null,null,"Nombre d'heures d'inconfort d'au moins +2°C (h)",null,113.5,110.5,107.5,113.5,110,107,113.5,110.5,107.5,113.5,null,107.5,113,null,null,113.5,110,null,113.5,110,null,115.5,null,110,113.5,110,null,113.5,null,null,null,null,null,113.5]
["Th-DC",null," Degrés-heures d'inconfort  (°C.h)",null,541.83505467975942,522.40209961385449,511.15648078499197,539.67036719397345,519.33557654582251,505.76258920166345,532.42071513886003,508.21846788953394,497.9668503819845,521.56287246955151,null,486.898665837951,537.85627024258349,null,null,554.68489372731449,535.42553746104295,null,536.71371579974448,514.69202401084101,null,562.84657652209853,null,533.85789083090651,556.70384342555803,538.61842221762697,null,523.4605428037255,null,null,null,null,null,536.08775164077701]
[null,null," Nombre d'heures d'inconfort total (h)",null,221.5,221,220,223,220.5,218.5,221,218,217.5,221,null,218.5,222,null,null,225.5,223.5,null,222.5,219.5,null,225,null,221.5,222.5,222,null,220.5,null,null,null,null,null,222.5]
[null,null,"Nombre d'heures d'inconfort d'au moins +1°C (h)",null,167.5,164.5,164.5,168.5,165,162.5,165.5,162,161,167,null,161.5,166.5,null,null,172,169,null,167,161.5,null,173.5,null,168,169,167,null,165,null,null,null,null,null,167.5]
[null,null,"Nombre d'heures d'inconfort d'au moins +2°C (h)",null,121.5,116.5,114,120,115.5,112.5,117.5,114,112,116,null,111,119.5,null,null,123.5,119.5,null,117,115.5,null,124,null,119.5,122,117.5,null,116.5,null,null,null,null,null,117]
[]
[]
[null,null,null,null,"Gaz  collectif",null,null,"Gaz collectif + CESC",null,null,"Gaz individuel",null,null,"Gaz indiv. + DF",null,null,"Gaz + CET collectif",null,null,"Bois",null,null,"PAC O/O DS",null,null,"EJ + CET air extrait",null,null,"RCU",null,null,"Gaz indiv. + CET extrait",null,null,"Gaz indiv. + CET extérieur",null,null,"PAC DS air/eau"]
["H2b",null,null,null,"V1",null,null,"V2",null,null,"V3",null,null,"V4",null,null,"V6",null,null,"V7",null,null,"V8",null,null,"V9",null,null,"V10",null,null,"V11",null,null,"V12 corrigé",null,null,"V13"]
[null,null,"Résultats - ENERGIE",null,"V1_Bbio_H2b","V1_Bbio20_H2b","V1_Bbio40_H2b","V2_Bbio_H2b","V2_Bbio20_H2b","V2_Bbio40_H2b","V3_Bbio_H2b","V3_Bbio20_H2b","V3_Bbio40_H2b","V4_Bbio_H2b","V4_Bbio20_H2b","V4_Bbio40_H2b","V6_Bbio_H2b","V6_Bbio20_H2b","V6_Bbio40_H2b","V7_Bbio_H2b","V7_Bbio20_H2b","V7_Bbio40_H2b","V8_Bbio_H2b","V8_Bbio20_H2b","V8_Bbio40_H2b","V9_Bbio_H2b","V9_Bbio20_H2b","V9_Bbio40_H2b","V10_Bbio_H2b","V10_Bbio20_H2b","V10_Bbio40_H2b","V11_Bbio_H2b","V11_Bbio20_H2b","V11_Bbio40_H2b","V12_Bbio_H2b","V12_Bbio20_H2b","V12_Bbio40_H2b","V13_Bbio_H2b","V13_Bbio20_H2b","V13_Bbio40_H2b"]
[null,"Cep (kWh/m2SREF par an)",null,null,98.576095601833899,93.203361338807497,86.720586813039006,88.816132836246894,83.367858543936094,76.741364694477198,90.706672968452395,85.299939967825196,78.905582001185707,95.745769735766899,90.140147776497102,83.679583815883802,91.074923082263496,85.55,78.900000000000006,102.07511694079599,96.156512984330305,null,73.3896965655548,70.8124902647818,null,135.734258457919,121.76736100833099,104.950438286105,112.948354706408,105.862325406515,null,95.261833356205202,89.534444633891596,null,98.517032179230299,92.836825956000993,86.252243971630406,77.744372947693705,74.236608342953602]
[null,"Cep_nr (kWh/m2SREF par an)",null,null,98.576095601833899,93.203361338807497,86.720586813039006,88.816132836246894,83.367858543936094,76.741364694477198,90.706672968452395,85.299939967825196,78.905582001185707,95.745769735766899,90.140147776497102,83.679583815883802,91.074923082263496,85.56,78.900000000000006,35.764326274303798,36.2630684049603,null,73.3896965655548,70.8124902647818,null,135.734258457919,121.76736100833099,104.950438286105,55.537309290483002,53.596548249412002,null,95.261833356205202,89.534444633891596,null,98.517032179230299,92.836825956000993,86.252243971630406,77.744372947693705,74.236608342953602]
[null,"RCR (%)",null,null,1.7321819781514199E-2,1.3772492038362699E-2,9.2093735645755702E-3,0.12396044223512701,0.12713714186445499,0.132258397167654,0,0,0,0.29949204546348301,0.31601587890527599,0.33835732116383799,0.109401035460802,0.111,0.115,0.63276787340351404,0.60538281291297602,null,0.31350667461765003,0.29786188797535801,null,1.6166731334146E-3,1.8083305261205099E-3,2.1111172102489398E-3,0.50640713359106604,0.491637117951432,null,1.17781982176751E-2,6.6385574537664903E-3,null,1.15013969930474E-2,6.50682994367675E-3,2.8198124004238201E-3,0.23414975323551401,0.22291202084787701]
["CH","Quantités d'énergie finale importées pour le chauffage (kWh/m2SREF)","Gaz",null,34.703931811846502,28.857849445926,21.628865494663401,34.768414597106599,28.8706814192129,21.763036305751498,35.969772546312001,30.122783857883199,23.1569687477316,37.460436424197503,31.519883136496802,24.146021571898999,35.244754053974397,29.28,22.14,0,0,null,0,0,null,0,0,0,0,0,null,36.223518160301303,30.168810250350301,null,36.223518160301303,30.168810250350301,23.166274413180801,0,0]
[null,null,"Bois",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,35.630000000000003,29.22,null,0,0,null,0,0,0,0,0,null,0,0,null,0,0,0,0,0]
[null,null,"Reseau",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,0,null,0,0,0,53.1888642970167,45.836663317371098,null,0,0,null,0,0,0,0,9.5584944977618402]
[null,null,"Elec importée",null,0.117762768168957,9.8649028498372496E-2,7.4510135377410802E-2,0.11885331880679199,9.9602963805188904E-2,7.5901753171756695E-2,0.40496725427307401,0.39013283251704201,0.35585196113437001,0.397775124249728,0.37201953226913598,0.29396649518948198,0.120280907031523,0.1,7.6999999999999999E-2,8.0370231811492304E-2,7.16702451214489E-2,null,9.5450835708237207,8.1822480686846095,null,34.488697322097799,28.18,20.7201675350837,0,0,null,0.41007273681391498,0.39501093753369798,null,0.41007273681391498,0.39501093753369798,0.36059196269405402,11.302962612696399,0]
["FR","Quantités d'énergie finale importées pour le refroidissement (kWh/m2SREF)","Gaz",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,0,null,0,0,0,0,0,null,0,0,null,0,0,0,0,0]
[null,null,"Reseau",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,0,null,0,0,0,0,0,null,0,0,null,0,0,0,0,5.9705210589047999]
[null,null,"Elec importée",null,5.8324418187009099,6.0706349358001299,6.4217621467394004,5.7746565212502601,6.0063528741477903,6.2714080138202402,5.6823960653928296,5.9149118672177998,6.1715785366488598,6.4259333751055401,6.6031550384469204,6.9437252633262103,5.7781768573501999,6.01,6.27,6.0018821947999896,6.2422951046572104,null,5.7538989951154997,5.98063358054792,null,6.0596267042653,6.3078120112121399,6.4864980714223197,5.1683726801230501,5.3060024816104301,null,5.5613056896527802,5.78219567513257,null,5.5613056896527802,5.78219567513257,6.0361302573669304,5.7346408685216002,0]
["ECS","Quantités d'énergie finale importées pour l'ECS (kWh/m2SREF)","Gaz",null,28.345362383705801,28.348044455544901,28.4161037418848,18.5943638975961,18.589306031043598,18.586294975332098,23.064586200933899,23.084638378428799,23.167085314189801,23.087033641220501,23.146630841332001,23.383599889616502,8.5856449383026394,8.58,8.58,0,0,null,0,0,null,0,0,0,0,0,null,0,0,null,0,0,0,0,0]
[null,null,"Bois",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,30.68,30.67,null,0,0,null,0,0,0,0,0,null,0,0,null,0,0,0,0,0]
[null,null,"Reseau",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,0,null,0,0,0,28.826914868589899,28.828732621348099,null,0,0,null,0,0,0,0,0]
[null,null,"Elec importée",null,9.3041737332319602E-2,9.3120737630238495E-2,9.3918477362288394E-2,0.116770451990251,0.11685279279130199,0.117555517305137,0.33246850376257497,0.33972139169603899,0.36511903805051898,0.34153102821916898,0.359673808955565,0.42860245708385702,5.2371607828596698,5.24,5.24,7.1377796985042694E-2,7.2308316258631905E-2,null,7.2039095862186802,7.2349243178962199,null,11.3087309064996,11.2933441565804,11.266035431305101,0,0,null,12.3433593307191,12.321337062800399,null,13.7586631668169,13.7571550289349,13.754907109497999,7.3585238281777503,7.3572866235234304]
[null,"Quantités d'énergie finale importées pour l'éclairage (kWh/m2SREF)",null,null,1.71459479132021,1.7148857875300101,1.71522238756742,1.7144960712124,1.71468309240723,1.7150601351536701,1.71423945318231,1.71464188395606,1.7148023505205301,1.71483851062436,1.7150380079202101,1.7151533409529001,1.71449525593911,1.7145999999999999,1.7150000000000001,1.71466623573277,1.7149538577163299,null,1.71447124612282,1.7146822770450201,null,1.7151390828359101,1.71507674923368,1.71510537442887,1.7131980301293801,1.7135014888737701,null,1.7140356768181799,1.7145710826001399,null,1.7140356768181799,1.7145710826001399,1.7147988030029599,1.7144250476243601,1.71468309240723]
[null,"Quantités d'énergie finale importées pour la ventilation (kWh/m2SREF)",null,null,1.1600487964961901,1.16010550761188,1.1601771095156601,1.1600313478666799,1.1600890779674999,1.1601598842032601,1.1600186084811701,1.1600786622093999,1.16013768924385,1.9348023183184699,1.9348802500127,1.9349203220978901,1.1600307962512,1.1599999999999999,1.1599999999999999,1.1600660391653099,1.1601173744367299,null,1.1600313478666799,1.1600885263245799,null,1.1600645858877701,1.16011882966889,1.1601825494273299,1.88557794433587E-3,1.8924680627873901E-3,null,1.1600167798566801,1.1600610016085799,null,1.1600167798566801,1.1600610016085799,1.16012283620613,1.1600188421759701,1.1600890779674999]
[null,"Quantités d'énergie finale importées pour la distribution (kWh/m2SREF)",null,null,2.2459091018993802,2.2310428496636399,2.19769646109817,2.2470602317897099,2.2319031138952998,2.1999039527544699,0.19384659425324499,0.15114700005860601,0.11575717913747301,0.20609364916092601,0.155916025177217,0.118372469876923,2.24831645087965,2.23,2.2000000000000002,2.2387106287048901,2.2225726261296801,null,2.24853503398458,2.2328260949414198,null,0,0,0,2.2828532189904802,2.2598495586382001,null,0.197406099893113,0.155333244355496,null,0.197406099893113,0.155333244355496,0.11949506783154699,2.2486937022923699,2.23307793425777]
[null,"Quantités d'énergie finale importées pour le déplacement des occupants (kWh/m2SREF)",null,null,4.2826363801175296,4.28263841658804,4.28263841658804,4.28263841658804,4.28263841658804,4.28263841658804,4.28263841658804,4.28263841658804,4.28263841658804,4.28263841658804,4.2826363801175296,4.28263841658804,4.2826363801175296,4.28,4.28,4.28263841658804,4.28263841658804,null,4.28263841658804,4.2826363801175296,null,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,null,4.2826363801175296,4.2826363801175296,null,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.28263841658804]
[null,"Production d'électricité en énergie finale par les installations photovoltaïques (kWh/m2SREF)","Elec produite",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,0,null,0,0,0,0,0,null,0,0,null,0,0,0,0,0]
[null,null,"Elec autoconsommée",null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0]
[null,"Quantité d'énergie anuelles importées par poste en énergie finale (kWh/m2SREF par an)","Chauffage",null,34.821694580015397,28.956512243759398,21.703385950385702,34.887284505435801,28.970298158908601,21.838948443730501,36.3747570974271,30.5129311998401,23.512831889634501,37.858229550706596,31.891902668766001,24.4399996887417,35.365034961005897,29.38,22.22,35.712884944857699,29.294132986462898,null,9.5450881096823696,8.1822480686846095,null,34.488697322097799,28.183342746374802,20.7201675350837,53.1888642970167,45.836663317371098,null,36.633590897115297,30.563821187883999,null,36.633590897115297,30.563821187883999,23.526866375874899,11.302962612696399,9.5584990429976298]
[null,null,"Refroidissement",null,5.8324418187009099,6.0706378224960602,6.4217652004026302,5.7746592672031296,6.0063557302764501,6.2714109959873703,5.6823987674742096,5.9149146798646202,6.1715814713452897,6.4259364307522597,6.6031550384469204,6.94372856519227,5.7781768573501999,6.01,6.27,6.0018850488027597,6.2422980729806303,null,5.7539017311978,5.98063358054792,null,6.0596267042653,6.3078120112121399,6.4864980714223197,5.1683726801230501,5.3060024816104301,null,5.5613056896527802,5.78219567513257,null,5.5613056896527802,5.78219567513257,6.0361302573669304,5.7346408685216002,5.9705238979947799]
[null,null,"ECS",null,28.438404121038101,28.441178717459898,28.510035776274599,18.711143247066801,18.706167718949299,18.703859386653999,23.3970658304161,23.4243709088285,23.532215542226101,23.428575810142899,23.5063046502875,23.8122136698302,13.8228057211623,13.82,13.81,30.749685354561901,30.743318703160099,null,7.2039130118070496,7.2349243178962199,null,11.3087309064996,11.2933441565804,11.266035431305101,28.826914868589899,28.828732621348099,null,12.3433593307191,12.321337062800399,null,13.7586631668169,13.7571550289349,13.754907109497999,7.3585238281777503,7.3572901220453399]
[null,null,"Eclairage",null,1.71459479132021,1.7148857875300101,1.71522238756742,1.7144960712124,1.71468309240723,1.7150601351536701,1.71423945318231,1.71464188395606,1.7148023505205301,1.71483851062436,1.7150380079202101,1.7151533409529001,1.71449525593911,1.71,1.7150000000000001,1.71466623573277,1.7149538577163299,null,1.71447124612282,1.7146822770450201,null,1.7151390828359101,1.71507674923368,1.71510537442887,1.7131980301293801,1.7135014888737701,null,1.7140356768181799,1.7145710826001399,null,1.7140356768181799,1.7145710826001399,1.7147988030029599,1.7144250476243601,1.71468309240723]
[null,null,"Aux. ventilation",null,1.1600487964961901,1.16010550761188,1.1601771095156601,1.1600313478666799,1.1600890779674999,1.1601598842032601,1.1600186084811701,1.1600786622093999,1.16013768924385,1.9348023183184699,1.9348802500127,1.9349203220978901,1.1600307962512,1.1599999999999999,1.1599999999999999,1.1600660391653099,1.1601173744367299,null,1.1600313478666799,1.1600885263245799,null,1.1600645858877701,1.16011882966889,1.1601825494273299,1.88557794433587E-3,1.8924680627873901E-3,null,1.1600167798566801,1.1600610016085799,null,1.1600167798566801,1.1600610016085799,1.16012283620613,1.1600188421759701,1.1600890779674999]
[null,null,"Aux. distribution",null,2.2459091018993802,2.2310428496636399,2.19769646109817,2.2470602317897099,2.2319031138952998,2.1999039527544699,0.19384659425324499,0.15114700005860601,0.11575717913747301,0.20609364916092601,0.155916025177217,0.118372469876923,2.24831645087965,2.23,2.2000000000000002,2.2387106287048901,2.2225726261296801,null,2.24853503398458,2.2328260949414198,null,0,0,0,2.2828532189904802,2.2598495586382001,null,0.197406099893113,0.155333244355496,null,0.197406099893113,0.155333244355496,0.11949506783154699,2.2486937022923699,2.23307793425777]
[null,null," Deplacement",null,4.2826363801175296,4.28263841658804,4.28263841658804,4.28263841658804,4.28263841658804,4.28263841658804,4.28263841658804,4.28263841658804,4.28263841658804,4.28263841658804,4.2826363801175296,4.28263841658804,4.2826363801175296,4.28,4.28,4.28263841658804,4.28263841658804,null,4.28263841658804,4.2826363801175296,null,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,null,4.2826363801175296,4.2826363801175296,null,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.28263841658804]
[null,null,"Total",null,78.495729589587796,72.857001345108898,65.990921301832202,68.777313087162497,63.072135308992401,56.171981215071298,72.804964767822099,67.160722751345304,60.489964538695801,75.851114686293599,70.089833020728094,63.247026473279902,64.371496422705903,58.59,51.66,81.860536668413303,75.660032037474295,null,31.908578897249299,30.7880392455573,null,59.014894981703897,52.942330873187501,45.6306253417848,95.464725052911405,88.229278316021905,null,61.892350854172598,55.979955634498701,null,63.307654690270397,57.415773600633202,50.594956829898003,33.801901281606,32.276801584258301]
[null,"Quantité d'énergie anuelles importées par type d'énergie en énergie finale (kWh/m2SREF par an)","Gaz",null,63.049294195552299,57.2059211039007,50.044993033829698,53.362803869662201,47.460010018332802,40.349350467915201,59.034386819143599,53.207447537396703,46.324076089841,60.547498856827303,54.666513977828799,47.529644062704101,43.830398992277097,37.86,30.71,0,0,null,0,0,null,0,0,0,0,0,null,36.223518160301303,30.168810250350301,null,36.223518160301303,30.168810250350301,23.166274413180801,0,0]
[null,null,"Bois",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,66.310822198464095,59.893473059778401,null,0,0,null,0,0,0,0,0,null,0,0,null,0,0,0,0,0]
[null,null,"Electricité",null,15.4464353940355,15.6510802412082,15.945928268002399,15.414509217500299,15.6121252906596,15.822630747156101,13.7705779486786,13.953275213948601,14.1658884488547,15.303615829466301,15.423319042899299,15.717382410575899,20.541097430428898,20.74,20.95,15.549714469949199,15.766558977695899,null,31.908578897249299,30.7880392455573,null,59.014894981703897,52.942330873187501,45.6306253417848,13.4489458873048,13.563882377302701,null,25.668832693871199,25.8111453841484,null,27.084136529969101,27.246963350282901,27.428682416717201,33.801901281606,32.276801584258301]
[null,null,"Réseau de chaleur",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,0,null,0,0,0,82.015779165606602,74.6653959387192,null,0,0,null,0,0,0,0,0]
["Th-B","Bbio chaud (KWh/m2SREF)",null,null,38.089731102848802,31.560979111058401,23.947560003280302,38.089729484837001,31.560978822053201,23.947559026871801,38.089729017250797,31.560978533048299,23.947559026871801,38.089729017250797,31.560979111058401,23.947559026871801,38.089731437433599,31.560979111058401,23.947559026871801,38.089729484837001,31.560979111058401,null,38.089729484837001,31.560979111058401,null,38.135700593053997,31.560979111058401,23.947559026871801,38.089729484837001,38.089729017250797,null,38.089729017250797,31.560979111058401,null,38.089729484837001,31.560979111058401,null,38.089729484837001,31.560979111058401]
[null,"Bbio froid (KWh/m2SREF)",null,null,12.141363050857001,13.146045170984801,14.5446602066766,12.141358719485201,13.146011075222299,14.5446339641344,12.1413549178392,13.1459360969664,14.5446339641344,12.1413549178392,13.146045170984801,14.5446339641344,12.141309848094901,13.146045170984801,14.5446339641344,12.141358719485201,13.146045170984801,null,12.141358719485201,13.146045170984801,null,12.1338828284853,13.146045170984801,14.5446339641344,12.141358719485201,12.1413549178392,null,12.1413549178392,13.146045170984801,null,12.141358719485201,13.146045170984801,null,12.141358719485201,13.146045170984801]
[null,"Bbio éclairage (KWh/m2SREF)",null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,0,null,0,0,0,0,0,null,0,0,null,0,0,null,0,0]
[null,"Bbio (points)",null,null,100.46218830741201,89.4140485640864,76.984440419913895,100.462176408644,89.413979794550897,76.984385982012498,100.46216787018,89.413829260029502,76.984385982012498,100.46216787018,89.4140485640864,76.984385982012498,100.462082571057,89.4140485640864,76.984385982012498,100.462176408644,89.4140485640864,null,100.462176408644,89.4140485640864,null,100.539166843079,89.4140485640864,76.984385982012498,100.462176408644,100.46216787018,null,100.46216787018,89.4140485640864,null,100.462176408644,89.4140485640864,null,100.462176408644,89.4140485640864]
["Th-DB",null," Degrés-heures d'inconfort  (°C.h)",null,488.58004905412452,466.12781463970055,449.64712480207299,490.11099042803852,463.81571943587346,450.05480504066554,488.3966232319525,464.18308557285695,450.331702237554,488.3966232319525,464.18308557285695,450.331702237554,488.30463003226703,464.40787799389398,449.44835667870052,490.11099042803852,463.81571943587346,null,490.11099042803852,463.81571943587346,null,496.71613281397248,477.34736418114755,461.49703312605595,490.11099042803852,463.81571943587346,null,488.3966232319525,464.18308557285695,null,488.3966232319525,464.18308557285695,null,490.11099042803852,463.81571943587346]
[null,null," Nombre d'heures d'inconfort total (h)",null,231,227,223.5,231,227.5,224,230.5,227.5,226,230.5,227.5,226,231,228.5,223.5,231,227.5,null,231,227.5,null,232,231.5,229,231,227.5,null,230.5,227.5,null,230.5,227.5,null,231,227.5]
[null,null,"Nombre d'heures d'inconfort d'au moins +1°C (h)",null,167,165,162.5,168.5,164,162,166.5,165,162.5,166.5,165,162.5,167,165,161.5,168.5,164,null,168.5,164,null,168,167.5,166.5,168.5,164,null,166.5,165,null,166.5,165,null,168.5,164]
[null,null,"Nombre d'heures d'inconfort d'au moins +2°C (h)",null,114,109,103.5,114,108.5,103.5,114,108.5,104,114,108.5,104,114,108.5,103.5,114,108.5,null,114,108.5,null,115.5,111.5,107,114,108.5,null,114,108.5,null,114,108.5,null,114,108.5]
["Th-DC",null," Degrés-heures d'inconfort  (°C.h)",null,526.96156971416747,502.49659290187003,488.16488545561799,522.00949881786505,498.22254419719297,484.02879918432745,510.67379544717102,484.59785606854905,473.13660245403099,497.96512690499401,477.5145886158125,462.56718486385944,522.30913648096498,496.91471717089348,482.9133044968105,539.15049761520504,515.72142421535852,null,519.55959705126247,495.11537412430948,null,546.87558448420953,526.4304747038135,514.57533184641795,541.83013316113352,517.78840952616645,null,498.90169914155501,473.99880617829899,null,498.90169914155501,473.99880617829899,null,519.44617256385447,494.28982863285052]
[null,null," Nombre d'heures d'inconfort total (h)",null,239,236.5,236,239,235,235.5,236.5,232.5,232.5,236,234.5,234.5,239,235.5,234,244,242,null,239,235,null,245,241.5,241.5,237,234,null,233.5,228.5,null,233.5,228.5,null,238.5,234.5]
[null,null,"Nombre d'heures d'inconfort d'au moins +1°C (h)",null,173.5,171,169,173.5,170,168.5,171.5,167,166.5,170,167.5,165.5,173.5,169,168,175.5,172.5,null,173.5,170,null,178.5,174.5,172.5,174,172,null,169.5,168.5,null,169.5,168.5,null,173.5,169]
[null,null,"Nombre d'heures d'inconfort d'au moins +2°C (h)",null,120.5,117.5,113.5,118,117,113,117,114,109.5,116,112,108,118,116,112.5,122,118,null,118,115.5,null,123.5,120.5,120,121.5,118.5,null,116,111,null,116,111,null,118,115]
[null,"Eges Energie (kgCO2/m²)",null,null,{"$f":"LC!E82*'CO2'!$C$6+LC!E83*'CO2'!$C$7+LC!E60*'CO2'!$C$11+LC!E63*'CO2'!$C$12+LC!E77*'CO2'!$C$14+LC!E67*'CO2'!$C$13+SUM(LC!E69:E71)*'CO2'!$C$16","v":15.311194104825111},{"$f":"LC!F82*'CO2'!$C$6+LC!F83*'CO2'!$C$7+LC!F60*'CO2'!$C$11+LC!F63*'CO2'!$C$12+LC!F77*'CO2'!$C$14+LC!F67*'CO2'!$C$13+SUM(LC!F69:F71)*'CO2'!$C$16","v":13.997560320540844},{"$f":"LC!G82*'CO2'!$C$6+LC!G83*'CO2'!$C$7+LC!G60*'CO2'!$C$11+LC!G63*'CO2'!$C$12+LC!G77*'CO2'!$C$14+LC!G67*'CO2'!$C$13+SUM(LC!G69:G71)*'CO2'!$C$16","v":12.3905403097171},{"$f":"LC!H82*'CO2'!$C$6+LC!H83*'CO2'!$C$7+LC!H60*'CO2'!$C$11+LC!H63*'CO2'!$C$12+LC!H77*'CO2'!$C$14+LC!H67*'CO2'!$C$13+SUM(LC!H69:H71)*'CO2'!$C$16","v":13.110356936011739},{"$f":"LC!I82*'CO2'!$C$6+LC!I83*'CO2'!$C$7+LC!I60*'CO2'!$C$11+LC!I63*'CO2'!$C$12+LC!I77*'CO2'!$C$14+LC!I67*'CO2'!$C$13+SUM(LC!I69:I71)*'CO2'!$C$16","v":11.782782416096003},{"$f":"LC!J82*'CO2'!$C$6+LC!J83*'CO2'!$C$7+LC!J60*'CO2'!$C$11+LC!J63*'CO2'!$C$12+LC!J77*'CO2'!$C$14+LC!J67*'CO2'!$C$13+SUM(LC!J69:J71)*'CO2'!$C$16","v":10.18178210977918},{"$f":"LC!K82*'CO2'!$C$6+LC!K83*'CO2'!$C$7+LC!K60*'CO2'!$C$11+LC!K63*'CO2'!$C$12+LC!K77*'CO2'!$C$14+LC!K67*'CO2'!$C$13+SUM(LC!K69:K71)*'CO2'!$C$16","v":14.297100775869096},{"$f":"LC!L82*'CO2'!$C$6+LC!L83*'CO2'!$C$7+LC!L60*'CO2'!$C$11+LC!L63*'CO2'!$C$12+LC!L77*'CO2'!$C$14+LC!L67*'CO2'!$C$13+SUM(LC!L69:L71)*'CO2'!$C$16","v":12.985864925759834},{"$f":"LC!M82*'CO2'!$C$6+LC!M83*'CO2'!$C$7+LC!M60*'CO2'!$C$11+LC!M63*'CO2'!$C$12+LC!M77*'CO2'!$C$14+LC!M67*'CO2'!$C$13+SUM(LC!M69:M71)*'CO2'!$C$16","v":11.436458833566288},{"$f":"LC!N82*'CO2'!$C$6+LC!N83*'CO2'!$C$7+LC!N60*'CO2'!$C$11+LC!N63*'CO2'!$C$12+LC!N77*'CO2'!$C$14+LC!N67*'CO2'!$C$13+SUM(LC!N69:N71)*'CO2'!$C$16","v":14.738595785969924},{"$f":"LC!O82*'CO2'!$C$6+LC!O83*'CO2'!$C$7+LC!O60*'CO2'!$C$11+LC!O63*'CO2'!$C$12+LC!O77*'CO2'!$C$14+LC!O67*'CO2'!$C$13+SUM(LC!O69:O71)*'CO2'!$C$16","v":13.410906248545286},{"$f":"LC!P82*'CO2'!$C$6+LC!P83*'CO2'!$C$7+LC!P60*'CO2'!$C$11+LC!P63*'CO2'!$C$12+LC!P77*'CO2'!$C$14+LC!P67*'CO2'!$C$13+SUM(LC!P69:P71)*'CO2'!$C$16","v":11.808555309790901},{"$f":"LC!Q82*'CO2'!$C$6+LC!Q83*'CO2'!$C$7+LC!Q60*'CO2'!$C$11+LC!Q63*'CO2'!$C$12+LC!Q77*'CO2'!$C$14+LC!Q67*'CO2'!$C$13+SUM(LC!Q69:Q71)*'CO2'!$C$16","v":11.279744657462377},{"$f":"LC!R82*'CO2'!$C$6+LC!R83*'CO2'!$C$7+LC!R60*'CO2'!$C$11+LC!R63*'CO2'!$C$12+LC!R77*'CO2'!$C$14+LC!R67*'CO2'!$C$13+SUM(LC!R69:R71)*'CO2'!$C$16","v":9.9362300000000001},{"$f":"LC!S82*'CO2'!$C$6+LC!S83*'CO2'!$C$7+LC!S60*'CO2'!$C$11+LC!S63*'CO2'!$C$12+LC!S77*'CO2'!$C$14+LC!S67*'CO2'!$C$13+SUM(LC!S69:S71)*'CO2'!$C$16","v":8.3264280000000017},{"$f":"LC!T82*'CO2'!$C$6+LC!T83*'CO2'!$C$7+LC!T60*'CO2'!$C$11+LC!T63*'CO2'!$C$12+LC!T77*'CO2'!$C$14+LC!T67*'CO2'!$C$13+SUM(LC!T69:T71)*'CO2'!$C$16","v":2.9943564672091463},{"$f":"LC!U82*'CO2'!$C$6+LC!U83*'CO2'!$C$7+LC!U60*'CO2'!$C$11+LC!U63*'CO2'!$C$12+LC!U77*'CO2'!$C$14+LC!U67*'CO2'!$C$13+SUM(LC!U69:U71)*'CO2'!$C$16","v":2.8155859032931305},{"$f":"LC!V82*'CO2'!$C$6+LC!V83*'CO2'!$C$7+LC!V60*'CO2'!$C$11+LC!V63*'CO2'!$C$12+LC!V77*'CO2'!$C$14+LC!V67*'CO2'!$C$13+SUM(LC!V69:V71)*'CO2'!$C$16","v":0},{"$f":"LC!W82*'CO2'!$C$6+LC!W83*'CO2'!$C$7+LC!W60*'CO2'!$C$11+LC!W63*'CO2'!$C$12+LC!W77*'CO2'!$C$14+LC!W67*'CO2'!$C$13+SUM(LC!W69:W71)*'CO2'!$C$16","v":2.2011008839692701},{"$f":"LC!X82*'CO2'!$C$6+LC!X83*'CO2'!$C$7+LC!X60*'CO2'!$C$11+LC!X63*'CO2'!$C$12+LC!X77*'CO2'!$C$14+LC!X67*'CO2'!$C$13+SUM(LC!X69:X71)*'CO2'!$C$16","v":2.1089765684490578},{"$f":"LC!Y82*'CO2'!$C$6+LC!Y83*'CO2'!$C$7+LC!Y60*'CO2'!$C$11+LC!Y63*'CO2'!$C$12+LC!Y77*'CO2'!$C$14+LC!Y67*'CO2'!$C$13+SUM(LC!Y69:Y71)*'CO2'!$C$16","v":0},{"$f":"LC!Z82*'CO2'!$C$6+LC!Z83*'CO2'!$C$7+LC!Z60*'CO2'!$C$11+LC!Z63*'CO2'!$C$12+LC!Z77*'CO2'!$C$14+LC!Z67*'CO2'!$C$13+SUM(LC!Z69:Z71)*'CO2'!$C$16","v":4.3141681649811963},{"$f":"LC!AA82*'CO2'!$C$6+LC!AA83*'CO2'!$C$7+LC!AA60*'CO2'!$C$11+LC!AA63*'CO2'!$C$12+LC!AA77*'CO2'!$C$14+LC!AA67*'CO2'!$C$13+SUM(LC!AA69:AA71)*'CO2'!$C$16","v":3.830663968018758},{"$f":"LC!AB82*'CO2'!$C$6+LC!AB83*'CO2'!$C$7+LC!AB60*'CO2'!$C$11+LC!AB63*'CO2'!$C$12+LC!AB77*'CO2'!$C$14+LC!AB67*'CO2'!$C$13+SUM(LC!AB69:AB71)*'CO2'!$C$16","v":3.2510040972039356},0,0,0,{"$f":"LC!AF82*'CO2'!$C$6+LC!AF83*'CO2'!$C$7+LC!AF60*'CO2'!$C$11+LC!AF63*'CO2'!$C$12+LC!AF77*'CO2'!$C$14+LC!AF67*'CO2'!$C$13+SUM(LC!AF69:AF71)*'CO2'!$C$16","v":9.8926085435631776},{"$f":"LC!AG82*'CO2'!$C$6+LC!AG83*'CO2'!$C$7+LC!AG60*'CO2'!$C$11+LC!AG63*'CO2'!$C$12+LC!AG77*'CO2'!$C$14+LC!AG67*'CO2'!$C$13+SUM(LC!AG69:AG71)*'CO2'!$C$16","v":8.5270525879538237},{"$f":"LC!AH82*'CO2'!$C$6+LC!AH83*'CO2'!$C$7+LC!AH60*'CO2'!$C$11+LC!AH63*'CO2'!$C$12+LC!AH77*'CO2'!$C$14+LC!AH67*'CO2'!$C$13+SUM(LC!AH69:AH71)*'CO2'!$C$16","v":0},{"$f":"LC!AI82*'CO2'!$C$6+LC!AI83*'CO2'!$C$7+LC!AI60*'CO2'!$C$11+LC!AI63*'CO2'!$C$12+LC!AI77*'CO2'!$C$14+LC!AI67*'CO2'!$C$13+SUM(LC!AI69:AI71)*'CO2'!$C$16","v":9.9846032929095347},{"$f":"LC!AJ82*'CO2'!$C$6+LC!AJ83*'CO2'!$C$7+LC!AJ60*'CO2'!$C$11+LC!AJ63*'CO2'!$C$12+LC!AJ77*'CO2'!$C$14+LC!AJ67*'CO2'!$C$13+SUM(LC!AJ69:AJ71)*'CO2'!$C$16","v":8.6203807557525671},{"$f":"LC!AK82*'CO2'!$C$6+LC!AK83*'CO2'!$C$7+LC!AK60*'CO2'!$C$11+LC!AK63*'CO2'!$C$12+LC!AK77*'CO2'!$C$14+LC!AK67*'CO2'!$C$13+SUM(LC!AK69:AK71)*'CO2'!$C$16","v":7.0419177470268624},{"$f":"LC!AL82*'CO2'!$C$6+LC!AL83*'CO2'!$C$7+LC!AL60*'CO2'!$C$11+LC!AL63*'CO2'!$C$12+LC!AL77*'CO2'!$C$14+LC!AL67*'CO2'!$C$13+SUM(LC!AL69:AL71)*'CO2'!$C$16","v":2.3487967702795283},{"$f":"LC!AM82*'CO2'!$C$6+LC!AM83*'CO2'!$C$7+LC!AM60*'CO2'!$C$11+LC!AM63*'CO2'!$C$12+LC!AM77*'CO2'!$C$14+LC!AM67*'CO2'!$C$13+SUM(LC!AM69:AM71)*'CO2'!$C$16","v":1.0877883113491738},{"$f":"LC!AN82*'CO2'!$C$6+LC!AN83*'CO2'!$C$7+LC!AN60*'CO2'!$C$11+LC!AN63*'CO2'!$C$12+LC!AN77*'CO2'!$C$14+LC!AN67*'CO2'!$C$13+SUM(LC!AN69:AN71)*'CO2'!$C$16","v":0}]
[null,null,null,"Option 1",10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10]
[null,null,null,"Option 2",12,12,12,12,12,12,12,12,12,12,12,12,12,12,12,12,12,12,12,12,12,12,12,12,12,12,12,12,12,12,12,12,12,12,12,12]
[null,null,null,"Option 3",7,7,7,7,7,7,7,7,7,7,7,7,7,7,7,7,7,7,7,7,7,7,7,7,7,7,7,7,7,7,7,7,7,7,7,7]
[]
[null,null,null,"Option 1 Cep",90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90]
[null,null,null,"Option 1 BBIO",80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80]
[null,null,null,"Option 2 Cep",80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80,80]
[null,null,null,"Option 2 BBIO",90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90,90]
[null,null,null,"Option 3 Cep",70,70,70,70,70,70,70,70,70,70,70,70,70,70,70,70,70,70,70,70,70,70,70,70,70,70,70,70,70,70,70,70,70,70,70,70]
[null,null,null,"Option 3 BBIO",75,75,75,75,75,75,75,75,75,75,75,75,75,75,75,75,75,75,75,75,75,75,75,75,75,75,75,75,75,75,75,75,75,75,75,75]
[]
[null,null,null,null,"Gaz  collectif",null,null,"Gaz collectif + CESC",null,null,"Gaz individuel",null,null,"Gaz indiv. + DF",null,null,"Gaz + CET collectif",null,null,"Bois",null,null,"PAC O/O DS",null,null,"EJ + CET air extrait",null,null,"RCU",null,null,"Gaz indiv. + CET extrait",null,null,"Gaz indiv. + CET extérieur",null,null,"PAC DS air/eau"]
["H3",null,null,null,"V1",null,null,"V2",null,null,"V3",null,null,"V4",null,null,"V6",null,null,"V7",null,null,"V8",null,null,"V9",null,null,"V10",null,null,"V11",null,null,"V12 corrigé",null,null,"V13"]
[null,null,"Résultats - ENERGIE",null,"V1_Bbio_H3","V1_Bbio20_H3","V1_Bbio40_H3","V2_Bbio_H3","V2_Bbio20_H3","V2_Bbio40_H3","V3_Bbio_H3","V3_Bbio20_H3","V3_Bbio40_H3","V4_Bbio_H3","V4_Bbio20_H3","V4_Bbio40_H3","V6_Bbio_H3","V6_Bbio20_H3","V6_Bbio40_H3","V7_Bbio_H3","V7_Bbio20_H3","V7_Bbio40_H3","V8_Bbio_H3","V8_Bbio20_H3","V8_Bbio40_H3","V9_Bbio_H3","V9_Bbio20_H3","V9_Bbio40_H3","V10_Bbio_H3","V10_Bbio20_H3","V10_Bbio40_H3","V11_Bbio_H3","V11_Bbio20_H3","V11_Bbio40_H3","V12_Bbio_H3","V12_Bbio20_H3","V12_Bbio40_H3","V13_Bbio_H3","V13_Bbio20_H3","V13_Bbio40_H3"]
[null,"Cep (kWh/m2SREF par an)",null,null,93.904073480442406,89.156459189282003,83.300749711327796,81.269170110490805,76.536354026016099,70.643578556943694,85.702909716502603,80.872760665860994,75.217156683613197,87.417850696222501,83.050657356966099,77.807454362898795,86.323508301230504,70.504133769650494,null,96.320561430006904,91.2471369106932,null,76.190101201512107,73.4907203717339,null,112.97443873704199,101.768780837647,88.858200281914804,104.00898301477901,98.469056572676706,null,89.174395454645904,84.352576743156007,null,90.952558646024798,86.1511905876349,80.165899449052404,76.724596791903807,73.404749798244794]
[null,"Cep_nr (kWh/m2SREF par an)",null,null,93.904073480442406,89.156459189282003,83.300749711327796,81.269170110490805,76.536354026016099,70.643578556943694,85.702909716502603,80.872760665860994,75.217156683613197,87.417850696222501,83.050657356966099,77.807454362898795,86.323508301230504,70.504133769650494,null,46.394432162954999,46.220757152399997,null,76.190101201512107,73.4907203717339,null,112.97443873704199,101.768780837647,88.858200281914804,61.3953313721413,59.389033415357098,null,89.174395454645904,84.352576743156007,null,90.952558646024798,86.1511905876349,80.165899449052404,76.724596791903807,73.404749798244794]
[null,"RCR (%)",null,null,6.8147811644912997E-3,3.4668079601129602E-3,0,0.163333783991613,0.16879605260014599,0.177282711798463,0,0,0,0.27037457234234102,0.28408588244042898,0.30615659511504101,0.10375327339266401,0.10811931748336499,null,0.49967067301695101,0.474633495442777,null,0.24355052593530099,0.229737530693055,null,1.8331122223420901E-3,2.0398568931352299E-3,2.35624295853493E-3,0.40721209420245102,0.39417697633685,null,3.7209480432637602E-3,2.51432379029695E-3,null,4.1084594901648896E-3,2.9425538339131999E-3,3.1609366575300101E-3,0.195141613468609,0.18485318888303601]
["CH","Quantités d'énergie finale importées pour le chauffage (kWh/m2SREF)","Gaz",null,21.8564993214593,17.2935773180007,11.6334839225353,21.856556288373,17.281636606414899,11.619553343469599,22.9676993141799,18.424876501198899,12.7480683378971,21.081507363862499,17.026787394514201,11.389731145265101,22.126829952204499,18.4660062957546,null,0,0,null,0,0,null,0,0,0,0,0,null,22.9051111332669,18.4660062957546,null,22.9051111332669,18.4660062957546,12.487285730815801,0,0]
[null,null,"Bois",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,22.036523969608702,17.141127344374699,null,0,0,null,0,0,0,0,0,null,0,0,null,0,0,0,0,0]
[null,null,"Reseau",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,0,null,6.3333012195427996,0,null,0,0,0,34.606425096807598,29.560501751795201,null,0,0,null,0,0,0,0,0]
[null,null,"Elec importée",null,7.501517675812E-2,6.0039521103384702E-2,4.1432171014567802E-2,7.5892542780047895E-2,6.08770810195709E-2,4.2422584138250397E-2,0.32696117577983602,0.313795285518572,0.295715020890921,0.313670867032732,0.30485435248631498,0.22184140522462001,7.6730067628207999E-2,0.318272874116731,null,5.7242175591989498E-2,5.0751398110271198E-2,null,0,5.2652329469170898,null,20.838201657113,16.028677395546701,10.366456155055101,0,0,null,0.33124597624371199,0.318272874116731,null,0.33124597624371199,0.318272874116731,0.29976871092653401,7.1702131679721397,5.8675398318189904]
["FR","Quantités d'énergie finale importées pour le refroidissement (kWh/m2SREF)","Gaz",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,0,null,0,0,null,0,0,0,0,0,null,0,0,null,0,0,0,0,0]
[null,null,"Reseau",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,0,null,0,0,null,0,0,0,0,0,null,0,0,null,0,0,0,0,0]
[null,null,"Elec importée",null,10.5875906330542,10.5314803171372,10.4911736576779,10.516351949196901,10.4758341296852,10.425528840202301,10.350766974142299,10.255650725469099,10.2853206461605,11.1466493551057,11.0393585604621,11.125000217229401,10.5198737323822,10.0907332065405,null,10.7703685806386,10.714783493663299,null,10.4812784433371,10.3560425207189,null,10.7737664578276,10.7214968028113,10.8056560703534,10.614113814475999,10.4147282210331,null,10.2018312395093,10.0907332065405,null,10.2018312395093,10.0907332065405,10.137702015171699,10.4690274796108,10.343222818440299]
["ECS","Quantités d'énergie finale importées pour l'ECS (kWh/m2SREF)","Gaz",null,25.9908068050945,26.0001476202182,26.0051522305737,13.4487592898888,13.449956580555799,13.4430453377449,20.739872883340801,20.763116329132199,20.7933573141522,20.7706183596854,20.778560828746699,21.038167127894301,7.5598121340657602,0,null,0,0,null,0,0,null,0,0,0,0,0,null,0,0,null,0,0,0,0,0]
[null,null,"Bois",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,27.889605297443101,27.885252413918501,null,0,0,null,0,0,0,0,0,null,0,0,null,0,0,0,0,0]
[null,null,"Reseau",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,0,null,7.0338952876088197,0,null,0,0,0,26.270220106960899,26.2681027586613,null,0,0,null,0,0,0,0,0]
[null,null,"Elec importée",null,8.6408927442246805E-2,8.6531678029652795E-2,8.6664313582955996E-2,0.11521613697434301,0.115376363343288,0.115512794468404,0.39089643534756502,0.39815278055794001,0.409027076204801,0.40177570235672599,0.40539676008286002,0.48159827654894399,4.7508630044442004,5.0554686147346599,null,7.4683075461647E-2,7.5241749077220602E-2,null,0,7.0677262354335504,null,10.4216032377629,10.4110569919584,10.375705899382099,0,0,null,11.086566873309501,11.076530777128401,null,11.8596813043438,11.858536796467,11.856422899950701,6.4415405483688604,6.4407210789695899]
[null,"Quantités d'énergie finale importées pour l'éclairage (kWh/m2SREF)",null,null,1.64256715404633,1.64290457900148,1.64258701447425,1.64256715404633,1.6428011549435699,1.64258701447425,1.6422971708060401,1.6425169004620399,1.6421346109003301,1.64280120654443,1.6425849028057899,1.64260423718425,1.64256715404633,1.6425169004620399,null,1.6426912391819,1.64291027456303,null,1.6425679351165099,1.6425169004620399,null,1.6426546582730399,1.6429139977329601,1.64300603237801,1.6418623253314699,1.6418757404764099,null,1.6422971708060401,1.6425169004620399,null,1.6422971708060401,1.6425169004620399,1.6422324789749001,1.64256715404633,1.6425169004620399]
[null,"Quantités d'énergie finale importées pour la ventilation (kWh/m2SREF)",null,null,1.16044126807059,1.1604914244732001,1.1605254060286201,1.1604284517985499,1.1604914244732001,1.16052452968725,1.1604270228357001,1.1604695130604801,1.1605053593238099,1.9352081056502,1.9352288471732799,1.93526793364927,1.1604284517985499,1.16045099293799,null,1.16047066574321,1.1605123831419399,null,1.16042900360312,1.16047880143511,null,1.1604587989240001,1.16051444820116,1.16053958528557,2.3555451136250201E-3,2.3774565263413199E-3,null,1.16042256965492,1.16045099293799,null,1.16042256965492,1.16045099293799,1.1605053593238099,1.1604284517985499,1.16047880143511]
[null,"Quantités d'énergie finale importées pour la distribution (kWh/m2SREF)",null,null,2.19002191872347,2.1762353397302401,2.14807390850364,2.1911919643163098,2.1770968746982402,2.1486051941855999,0.104857240528364,7.0590517218603696E-2,4.4543963603792397E-2,8.84431539207573E-2,6.1813733265648201E-2,4.1293328193558E-2,2.1916256508700598,7.5193845827873806E-2,null,2.1834001280281901,2.16914569193536,null,2.1920250630748401,2.1778533330609999,null,0,0,0,2.2122222875747601,2.1977091854205399,null,0.10773210400205301,7.5193845827873806E-2,null,0.10773210400205301,7.5193845827873806E-2,4.6216380855110498E-2,2.1921071623917898,2.1779927966889501]
[null,"Quantités d'énergie finale importées pour le déplacement des occupants (kWh/m2SREF)",null,null,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,null,4.2826363801175296,4.2826363801175296,null,4.28263841658804,4.2826363801175296,null,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,null,4.2826363801175296,4.2826363801175296,null,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296]
[null,"Production d'électricité en énergie finale par les installations photovoltaïques (kWh/m2SREF)","Elec produite",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,0,null,0,0,null,0,0,0,0,0,null,0,0,null,0,0,0,0,0]
[null,null,"Elec autoconsommée",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0]
[null,"Quantité d'énergie anuelles importées par poste en énergie finale (kWh/m2SREF par an)","Chauffage",null,21.9315144982174,17.353616839104099,11.6749160935499,21.932448831153099,17.342513687434501,11.6619759276078,23.2946604899597,18.7386717867175,13.043783358788,21.395178230895201,17.331641747000599,11.611572550489701,22.2035600198327,18.784279169871301,null,22.0937661452007,17.191878742484999,null,6.3333042311412697,5.2652329469170898,null,20.838201657113,16.028677395546701,10.366456155055101,34.606425096807598,29.560501751795201,null,23.2363571095106,18.784279169871301,null,23.2363571095106,18.784279169871301,12.787054441742301,7.1702131679721397,5.8675398318189904]
[null,null,"Refroidissement",null,10.5875906330542,10.5314803171372,10.4911736576779,10.516351949196901,10.4758341296852,10.425528840202301,10.350766974142299,10.255650725469099,10.2853206461605,11.1466493551057,11.0393585604621,11.125000217229401,10.5198737323822,10.0907332065405,null,10.7703685806386,10.714783493663299,null,10.481283427373199,10.3560425207189,null,10.7737664578276,10.7214968028113,10.8056560703534,10.614113814475999,10.4147282210331,null,10.2018312395093,10.0907332065405,null,10.2018312395093,10.0907332065405,10.137702015171699,10.4690274796108,10.343222818440299]
[null,null,"ECS",null,26.0772157325367,26.086679298247802,26.0918165441566,13.563975426863101,13.565332943899101,13.5585581322133,21.130769318688401,21.161269109690199,21.202384390357,21.172394062042098,21.1839575888295,21.519765404443199,12.31067513851,5.0554686147346599,null,27.964288372904701,27.960494162995801,null,7.03389863235234,7.0677262354335504,null,10.4216032377629,10.4110569919584,10.375705899382099,26.270220106960899,26.2681027586613,null,11.086566873309501,11.076530777128401,null,11.8596813043438,11.858536796467,11.856422899950701,6.4415405483688604,6.4407210789695899]
[null,null,"Eclairage",null,1.64256715404633,1.64290457900148,1.64258701447425,1.64256715404633,1.6428011549435699,1.64258701447425,1.6422971708060401,1.6425169004620399,1.6421346109003301,1.64280120654443,1.6425849028057899,1.64260423718425,1.64256715404633,1.6425169004620399,null,1.6426912391819,1.64291027456303,null,1.6425679351165099,1.6425169004620399,null,1.6426546582730399,1.6429139977329601,1.64300603237801,1.6418623253314699,1.6418757404764099,null,1.6422971708060401,1.6425169004620399,null,1.6422971708060401,1.6425169004620399,1.6422324789749001,1.64256715404633,1.6425169004620399]
[null,null,"Aux. ventilation",null,1.16044126807059,1.1604914244732001,1.1605254060286201,1.1604284517985499,1.1604914244732001,1.16052452968725,1.1604270228357001,1.1604695130604801,1.1605053593238099,1.9352081056502,1.9352288471732799,1.93526793364927,1.1604284517985499,1.16045099293799,null,1.16047066574321,1.1605123831419399,null,1.16042900360312,1.16047880143511,null,1.1604587989240001,1.16051444820116,1.16053958528557,2.3555451136250201E-3,2.3774565263413199E-3,null,1.16042256965492,1.16045099293799,null,1.16042256965492,1.16045099293799,1.1605053593238099,1.1604284517985499,1.16047880143511]
[null,null,"Aux. distribution",null,2.19002191872347,2.1762353397302401,2.14807390850364,2.1911919643163098,2.1770968746982402,2.1486051941855999,0.104857240528364,7.0590517218603696E-2,4.4543963603792397E-2,8.84431539207573E-2,6.1813733265648201E-2,4.1293328193558E-2,2.1916256508700598,7.5193845827873806E-2,null,2.1834001280281901,2.16914569193536,null,2.1920250630748401,2.1778533330609999,null,0,0,0,2.2122222875747601,2.1977091854205399,null,0.10773210400205301,7.5193845827873806E-2,null,0.10773210400205301,7.5193845827873806E-2,4.6216380855110498E-2,2.1921071623917898,2.1779927966889501]
[null,null," Deplacement",null,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,null,4.2826363801175296,4.2826363801175296,null,4.28263841658804,4.2826363801175296,null,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,null,4.2826363801175296,4.2826363801175296,null,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296,4.2826363801175296]
[null,null,"Total",null,67.871987584766202,63.234044177811597,57.4917290045085,55.289600157491797,50.646706595251302,44.880416018488098,61.966414597078,57.311804932735399,51.661308709251003,61.663310494275997,57.477221759654498,52.158140051306901,54.311366527557396,41.091279110491897,null,70.097621511814907,65.1223611289019,null,33.126146709249298,31.9524871181452,null,49.119321190018098,44.247296016368097,38.634000122571599,79.629835556381806,74.367931494030501,null,51.717843446909903,47.112341272885701,null,52.490957877944197,47.894347292224303,41.912769956136003,33.358520344306001,31.915108607932499]
[null,"Quantité d'énergie anuelles importées par type d'énergie en énergie finale (kWh/m2SREF par an)","Gaz",null,47.847306126553697,43.293724938218901,37.638636153108997,35.305315578261798,30.731593186970699,25.062598681214499,43.707572197520697,39.187992830331197,33.541425652049298,41.8521257235479,37.8053482232609,32.4278982731594,29.6866420862703,18.4660062957546,null,0,0,null,0,0,null,0,0,0,0,0,null,22.9051111332669,18.4660062957546,null,22.9051111332669,18.4660062957546,12.487285730815801,0,0]
[null,null,"Bois",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,49.926129267051799,45.026379758293203,null,0,0,null,0,0,0,0,0,null,0,0,null,0,0,0,0,0]
[null,null,"Electricité",null,20.024681458212498,19.9403192395927,19.853092851399499,19.98428457923,19.9151134082806,19.817817337273599,18.258842399557398,18.123812102404301,18.119883057201701,19.811184770728101,19.671873536393498,19.730241778147601,24.624724441287,22.6252728147374,null,20.171492244763101,20.095981370608701,null,33.126146709249298,31.9524871181452,null,49.119321190018098,44.247296016368097,38.634000122571599,18.753190352613402,18.539326983574,null,28.8127323136431,28.646334977131101,null,29.585846744677401,29.4283409964697,29.4254842253203,33.358520344306001,31.915108607932499]
[null,null,"Réseau de chaleur",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,0,null,0,0,null,0,0,0,60.876645203768497,55.828604510456501,null,0,0,null,0,0,0,0,0]
["Th-B","Bbio chaud (KWh/m2SREF)",null,null,23.3631625726347,18.8451870273358,12.4233543013431,23.363158260602901,18.845176676625801,12.4233502159751,23.363153948544099,18.8451663211458,12.4233461750571,23.363153948544099,18.8451663211458,12.4233461750571,23.363228543553699,18.8451663211458,null,23.363158260602901,18.8451663211458,null,23.363158260602901,18.8451663211458,null,23.397129558245599,18.8451663211458,12.4233461750571,23.363158260602901,18.8451663211458,null,23.363153948544099,18.8451663211458,null,23.363153948544099,18.8451663211458,null,23.363158260602901,18.8451663211458]
[null,"Bbio froid (KWh/m2SREF)",null,null,27.8110053267274,27.7101963813213,28.786434770513701,27.8110040095366,27.710196005182102,28.786434758913401,27.811002692331801,27.925547112092101,28.786434746460198,27.811002692331801,27.925547112092101,28.786434746460198,27.811017617113201,27.925547112092101,null,27.8110040095366,27.925547112092101,null,27.8110040095366,27.925547112092101,null,27.805745788645702,27.925547112092101,28.786434746460198,27.8110040095366,27.925547112092101,null,27.811002692331801,27.925547112092101,null,27.811002692331801,27.925547112092101,null,27.8110040095366,27.925547112092101]
[null,"Bbio éclairage (KWh/m2SREF)",null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,0,null,0,0,null,0,0,0,0,0,null,0,0,null,0,0,null,0,0]
[null,"Bbio (points)",null,null,102.34833579872399,93.1107668173142,82.419578143713593,102.34832454027899,93.110745363615806,82.419569949776999,102.348313281752,93.541426866475703,82.4195618430347,102.348313281752,93.541426866475703,82.4195618430347,102.34849232133401,93.541426866475703,null,102.34832454027899,93.541426866475703,null,102.34832454027899,93.541426866475703,null,102.40575069378301,93.541426866475703,82.4195618430347,102.34832454027899,93.541426866475703,null,102.348313281752,93.541426866475703,null,102.348313281752,93.541426866475703,null,102.34832454027899,93.541426866475703]
["Th-DB",null," Degrés-heures d'inconfort  (°C.h)",null,1319.30566748097,1272.5863337047849,1245.5617865086201,1317.1464902421849,1273.4117053421151,1245.86750098315,1317.1092799994299,1270.7541996720452,1243.7505527158901,1317.1092799994299,1270.7541996720452,1243.7505527158901,1317.160456399625,1270.7541996720452,null,1317.1464902421849,1273.4117053421151,null,1317.1464902421849,1273.4117053421151,null,1320.9072157806349,1268.423592941685,1240.1622141662201,1317.1464902421849,1273.4117053421151,null,1317.1092799994299,1270.7541996720452,null,1317.1092799994299,1270.7541996720452,null,1317.1464902421849,1273.4117053421151]
[null,null," Nombre d'heures d'inconfort total (h)",null,790.5,778,775,789.5,778,775,789.5,777,774,789.5,777,774,790,777,null,789.5,778,null,789.5,778,null,790,777.5,774,789.5,778,null,789.5,777,null,789.5,777,null,789.5,778]
[null,null,"Nombre d'heures d'inconfort d'au moins +1°C (h)",null,511,496.5,486.5,510,497.5,486.5,510,495.5,485,510,495.5,485,510,495.5,null,510,497.5,null,510,497.5,null,511.5,493,485,510,497.5,null,510,495.5,null,510,495.5,null,510,497.5]
[null,null,"Nombre d'heures d'inconfort d'au moins +2°C (h)",null,264,250,241,264,250,241,264,250,241,264,250,241,264,250,null,264,250,null,264,250,null,263.5,247.5,238.5,264,250,null,264,250,null,264,250,null,264,250]
["Th-DC",null," Degrés-heures d'inconfort  (°C.h)",null,1403.6596174991801,1358.354820246175,1337.889506803635,1395.4186538879001,1350.1272134435999,1327.52915572755,1368.5706792045701,1326.2937144283801,1298.94604372039,1369.40149799393,1325.4265432121301,1300.9326880568701,1396.2766923668451,1301.0620087607549,null,1426.5911843076001,1385.3089640287499,null,1389.85323949654,1341.760278196575,null,1444.457633394675,1400.7557818739401,1382.5471472700751,1400.0468043574051,1352.14939483535,null,1346.0822964357299,1301.0620087607549,null,1346.0822964357299,1301.0620087607549,null,1386.96869803097,1339.07532525943]
[null,null," Nombre d'heures d'inconfort total (h)",null,825.5,814,810,824,811,806,812.5,801,798,818,810,801.5,824,789.5,null,836,826,null,822,810,null,836.5,828.5,828,819.5,806,null,806.5,789.5,null,806.5,789.5,null,820,806.5]
[null,null,"Nombre d'heures d'inconfort d'au moins +1°C (h)",null,535.5,527,517.5,532,524,514,529.5,514,502,528.5,515.5,505.5,531.5,505,null,541.5,532.5,null,530.5,520.5,null,548.5,536,528.5,537.5,523,null,523,505,null,523,505,null,530.5,520]
[null,null,"Nombre d'heures d'inconfort d'au moins +2°C (h)",null,286,273.5,268,284,271,267.5,279,265.5,260,278.5,267,262,284,260,null,291,280.5,null,281,268.5,null,298,286.5,277,282.5,272.5,null,270.5,260,null,270.5,260,null,280.5,268.5]

{"sheet":"Graph LC","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"CO2","index":4,"n_rows":16,"n_cols":3,"rows_kept":16,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[null,"CO2","kgCO2/kWh"]
[null,"Gaz",0.22700000000000001]
[null,"Bois granulés",0.03]
[null,"Bois plaquettes",2.4E-2]
[null,"Réseau chaud","selon réseau"]
[null,"Réseau froid","selon réseau"]
[null,"Electricité chauffage",7.9000000000000001E-2]
[null,"Electricité climatisation",6.4000000000000001E-2]
[null,"Electricité ECS",6.5000000000000002E-2]
[null,"Electricité éclairage résidentiel",6.9000000000000006E-2]
[null,"Electricité éclairage tertiare",6.4000000000000001E-2]
[null,"Electricté autres usages",6.4000000000000001E-2]